SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( DR_50_3520_Tender
 Type ( Tender )
 WagonShape ( DR_50_3520_Tender.s )
 Name ( "DR_50_3520_Tender" )
 Size ( 3.05m 4.11m 9.05m )
 CentreOfGravity ( 0m 1.90m 0m )
 Mass ( 59.5t )
 InertiaTensor ( Box (3.05m 4.11m 9.05m ) )

 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 2e6N/m 2e6N/m )
   Damping ( 0.5e5N/m/s 0.5e5N/m/s )
   Break ( 5e7N 5e7N )
   r0 ( 5cm 10cm )
  )
  CouplingHasRigidConnection ( 1 )
  Velocity ( 0.1m/s )
 )
 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 2e6N/m 2e6N/m )
   Damping ( 0.5e5N/m/s 0.5e5N/m/s )
   Break ( 5e7N 5e7N )
   r0 ( 10cm 20cm )
  )
  CouplingHasRigidConnection ()
  Velocity ( 0.1m/s )
 )
 

 Adheasion ( 0.2 0.4 2 0 )
 DerailRailHeight ( 4cm )
 DerailRailForce ( 7.5*59t )
 DerailBufferForce ( 400kN )
 WheelRadius ( 0.5m )
 NumWheels ( 4  )

 Friction (
  762N/m/s  0  1mph  3.14N/m/s 1.8
  5.1N/rad/s  1  -1rad/s  0  1
 )

 MaxBrakeForce ( 50kN )

 BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir" )

 BrakeSystemType ("Air_single_pipe")
 TripleValveRatio( 2.5 )
 MaxReleaseRate( 30 )
 MaxApplicationRate( 30 )
 MaxAuxilaryChargingRate( 145 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 54 )
 IntakePoint ( -3.5 0.5 FuelWater )
 IntakePoint ( 0.6 2.73 FuelCoal )
 
 Sound  ( "..//..//Common.snd//Sound_23.10//Tender.sms" )

 Lights ( 1
  Light (
   comment( tail light right )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 3 )
    Coupling (0)
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0215 )
     Position ( 0.85 1.48 -4.02 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 0.8 )
     )
    )
             )
       )
)
