SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( DR_50_3632_DT
	Comment (
		Created with EngMexx V1.0.2

	)
	Type ( Engine )
	WagonShape ( "DR_50.35.s" )
	Size ( 3.2m 4.6m 15.6m )
	CentreOfGravity ( 0m 1.7m 0m )
	Mass ( 88.2t )
	WheelRadius ( 0.425m )
	InertiaTensor ( Box ( 3.2m 4.6m 15.6m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1E6N/m 5E6N/m )
			Damping ( 1E6N/m/s 1E6N/m/s )
			Break ( 3.1E7N 3.1E7N )
			r0 ( -200cm -220cm )
		)
		CouplingHasRigidConnection (  )
		Velocity ( 0.1m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1E6N/m 5E6N/m )
			Damping ( 1E6N/m/s 1E6N/m/s )
			Break ( 3.1E7N 3.1E7N )
			r0 ( 20cm 30cm )
		)
		CouplingHasRigidConnection (  )
		Velocity ( -0.1m/s )
	)
	Adheasion ( 0.03 0.35 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 300kN )
	DerailBufferForce ( 300kN )
	NumWheels ( 2 )
	Friction (
		1189N/m/s	0	1mph	7.62N/m/s	1.8
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)
	BrakeEquipmentType ( "handbrake,triple_valve,auxilary_reservoir,emergency_brake_reservoir" )
	BrakeSystemType ( Air_single_pipe )
	MaxBrakeForce ( 120kN )
	EmergencyBrakeResMaxPressure ( 100 )
	TripleValveRatio ( 2.5 )
	MaxReleaseRate ( 5 )
	MaxApplicationRate ( 8 )
	MaxAuxilaryChargingRate ( 5 )
	EmergencyResCapacity ( 7 )
	EmergencyResChargingRate ( 5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 55 )
	MaxHandbrakeForce ( 80kN )
	NumberOfHandbrakeLeverSteps ( 100 )
	FreightAnim ( "DR_50_3632_Det.s" 1 1 )
	Inside (
		PassengerCabinFile ( "DR_50.35.s" )
		PassengerCabinHeadPos ( -1.6m 3.25m -5.6m )
		RotationLimit ( 0 180 0 )
		StartDirection ( 0 0 0 )
	)
	Lights ( 9
		Light (
			comment ( Licht #1 )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 3F808040 )
					Position ( 1 1.5 2.85 )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 3 )
				)
			)
		)
		Light (
			comment ( Licht #2 )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE0A0 )
					Position ( 1.35 1.98 2.85 )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( Licht #3 )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 3F808040 )
					Position ( -1 1.5 2.85 )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 3 )
				)
			)
		)
		Light (
			comment ( Licht #4 )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE0A0 )
					Position ( -1.35 1.98 2.52 )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light (
			comment ( Lichtkegel #5 )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 00808040 )
					Position ( 0 3 -10 )
					Angle ( 12 )
					Transition ( 0 )
					Radius ( 100 )
				)
			)
		)
		Light (
			comment ( Licht #6 )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE0A0 )
					Position ( 0 3.80 6.25 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.35 )
				)
			)
		)
		Light (
			comment ( Licht #7 )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE0A0 )
					Position ( 0.85 1.55 7.25 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.35 )
				)
			)
		)
		Light (
			comment ( Licht #8 )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE0A0 )
					Position ( -0.85 1.55 7.25 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.35 )
				)
			)
		)
		Light (
			comment ( Licht #9 )
			Type ( 0 )
			FadeIn ( 0 )
			FadeOut ( 0 )
			Cycle ( 0 )
			States ( 2
				State (
					Duration ( 0.05 )
					LightColour ( 80FF7200 )
					Position ( 0 1.2 -4 )
					Azimuth ( 0 -90 90 )
					Elevation ( 0 0 0 )
					Transition ( 0 )
					Radius ( 3.5 )
				)
				State (
					Duration ( 0.05 )
					LightColour ( 80FFE610 )
					Position ( 0 1.2 -4 )
					Azimuth ( 0 -90 90 )
					Elevation ( 0 0 0 )
					Transition ( 0 )
					Radius ( 3.5 )
				)
			)
		)
	)
	Sound ( "..//..//Common.snd//Sound_23.10//BR2310Eng.sms" )
)

Engine ( DR_50_3632_DT
	Effects (
		SteamSpecialEffects (
			WhistleFX ( 0.5 3.9 0.8 0 1 0 0.3 )
			SafetyValvesFX ( 0 4.2 -2.15 0 1 0 0.3 )
			StackFX ( 0 4.6 4.2 0 0.8 0 0.3 )
			CylindersFX ( -1.2 0.3 4.2 -0.5 -1 0 0.2 )
			CylindersFX ( 1.2 0.3 4.2 0.5 -1 0 0.2 )
		)
	)

	Wagon ( "DR_50_3632_DT" )
	Type ( Steam )
	MaxPower ( 1625hp )
	MaxForce ( 217kN )
	MaxVelocity ( 80km/h )
	WheelRadius ( 0.7m )
	Sanding ( 10mph )
	MaxSandingTime ( -1 )
	NumWheels ( 3 )

	HeadOut ( 1.7m 3.2m -5.6m )

	AirBrakesAirCompressorPowerRating ( 2 )
	AirBrakesAirCompressorWattage ( 8000 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 1.2 )
	AirBrakesCompressorRestartPressure ( 135 )
	AirBrakesIsCompressorElectricOrMechanical ( 1 )
	AirBrakesMainMaxAirPressure ( 174 )
	AirBrakesMainMinResAirPressure ( 104 )
	AirBrakesMainResVolume ( 10 )
	EngineBrakesControllerMinPressureReduction ( 6 )
	EngineBrakesControllerMaxApplicationRate ( 40 )
	EngineBrakesControllerMaxReleaseRate ( 40 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 55 )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	EngineBrakesControllerFullServicePressureDrop ( 26 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	TrainBrakesControllerMinPressureReduction ( 5 )
	TrainBrakesControllerMaxApplicationRate ( 8 )
	TrainBrakesControllerMaxReleaseRate ( 5 )
	TrainBrakesControllerEmergencyApplicationRate ( 30 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 72.5 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )
	BrakesEngineBrakeType ( Air_single_pipe )
	BrakesTrainBrakeType ( Air_single_pipe )
	BrakesEngineControllers ( "Train,Independent,Hand" )
	Cabview ( BR50SSR.cvf )

	BasicCoalUsage ( 600lb/h )
	BasicSteamUsage ( 3000lb/h )
	BlastExponent ( 0.9 )
	BoilerEffectivity ( 1 )
	BoilerLength ( 2.2m )
	BoilerResponsiveness ( 1 )
	CoalBurnage ( 5lb/hp/h )
	CutoffMaxForward ( 0.85 )
	CutoffMaxReverse ( -0.85 )
	CylinderCocksPowerEfficiency ( 0.85 )
	CylinderDiameter ( 0.6m )
	CylinderEffectivity ( 1 )
	CylinderStroke ( 0.66m )
	CylinderVolume ( "0.37*(m^3)" )
	DraftingEffect ( 0.85 )
	ExhaustLimit ( 22000lb/h )
	IdealFireMass ( 1300lb )
	InjectorSizes ( 25mm 35mm )
	InjectorTypes ( 0 1 )
	Injector1FeedRateMultiplierLive ( 0.25 )
	Injector2FeedRateMultiplierExhaust ( 0.5 )
	Injector1WaterValveVariance ( 0.5 )
	Injector2WaterValveVariance ( 0.5 )
	InjectorLimits1 ( 60 0.5 1 )
	InjectorLimits2 ( 80 0.6 1 )
	IsTenderRequired ( 1 )
	MaxBoilerOutput ( 25000lb/h )
	MaxBoilerPressure ( 232.060289263151 )
	MaxFireMass ( 2200lb )
	MaxSteamHeatingPressure ( 60 )
	MaxTenderCoalMass ( 8t )
	MaxTenderWaterMass ( 23t )
	MaxWaterMass ( 7.5t )
	NumCylinders ( 2 )
	PrimingFactor ( 1 )
	RegulatorMainValveInitialOpenning ( 0.495 )
	RegulatorPilotValveExponent ( 1.75 )
	RegulatorPilotValveFullOpenning ( 0.49 )
	RegulatorSecondValveExponent ( 1.7 )
	RegulatorSecondValveStartPosition ( 0.1 )
	RegulatorValveType ( single_port )
	SafetyValvePressureDifference ( 10 )
	SafetyValvesSteamUsage ( 30000lb/h )
	SteamBlowerEffectExponent ( 1.1 )
	SteamBlowerEfficiencyExponent ( 1.1 )
	SteamBlowerMaxProportionOfBlastEffect ( 0.3 )
	SteamBlowerMaxSteamUsageRate ( 1900 )
	SteamCylinderCocksOperation ( manual )
	SteamFiremanMaxPossibleFiringRate ( 6000 )
	SteamGaugeGlassHeight ( 16 )
	SteamMaxSmokeUnitsReleaseRate ( 30 )
	SteamSmallestCutoff ( 3 )
	SteamSmokeUnitsPerPoundOfFuel ( 0.9 )
	SuperHeater ( 1.22 )


	EngineControllers (
		BellToggle ( 0 1 0 )
		Blower ( 0 1 0.05 0.1
			NumNotches ( 0 )
		)
		Brake_Engine ( 0 1 0.04 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Train ( 0 1 0.02 0.35
			NumNotches ( 3
				Notch ( 0 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.3 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.98 0 TrainBrakesControllerContinuousServiceStart )
			)
		)
		Cutoff ( -0.85 0.85 0.05 0
			NumNotches ( 0 )
		)
		CylinderCocks ( 0 1 1 )
		DampersFront ( 0 1 0.05 1
			NumNotches ( 2
				Notch ( 0 0 Dummy )
				Notch ( 0.7 1 Dummy )
			)
		)
		DampersBack ( 0 16 1 10
			NumNotches ( 0 )
		)
		Firedoor ( 0 1 1 0
			NumNotches ( 0 )
		)
		Headlights ( 0 1 0 )
		HeatingTap ( 0 1 0.05 0
			NumNotches ( 0 )
		)
		Injector1Steam ( 0 1 0 )
		Injector1Water ( 0 1 0.1 1
			NumNotches ( 0 )
		)
		Injector2Steam ( 0 1 0 )
		Injector2Water ( 0 1 0.1 1
			NumNotches ( 0 )
		)
		Regulator ( 0 1 0.06 0
			NumNotches ( 0 )
		)
		Sanding ( 0 1 0 )
		Shovel ( 0 1 0.1 0
			NumNotches ( 0 )
		)
		SmallEjectorOrCompressor ( 0 1 1 )
		Whistle ( 0 1 0 )
	)

	Name ( "DR_50_3632_DT_Bw_Blankenburg" )
	Sound ( "..//..//Common.snd//Sound_23.10//BR2310Cab.sms" )

	EngineVariables ( 950 1500 7000 230 20000 6000 400 1 0.9 )

	Description (
		"Ab 1957 erhielten im RAW Dessau zahlreiche 50er Lokomotiven einen Ersatzkessel und wurden in die Gattung BR50.35 eingeordnet Die BR50.35 ist sowohl im Güterzug- als auch im Personenzugdienst eingesetzt. Beachtenswert ist, daß mit dem gekuppelten Tender T26 auch bei Rückwärtsfahrt die Höchtsge- schwindigkeit von 80 Kmh gefahren werden kann. Somit ist diese Lok auch öfters auf Nebenstrecken (meist ohne Wendemöglichkeit) eingesetzt worden."
	)
	EngineOperatingProcedures (
		"..."
	)
)
