SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( DR_52_1331_DT
	Type ( Engine )
	WagonShape ( DR_52_1331.s )
	FreightAnim( DR_52_1331_Details.s 1 1 )
	Size ( 3.07m 4.4m 13.90m  )
	CentreOfGravity ( 0m 1.7m 0m )
	Centre ( 0m 0m 0m )
	Mass ( 84t )
	InertiaTensor ( Box(3.07m 4.4m 13.684m) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 4e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5e7N 5e7N )
			r0 ( 10cm 40cm )
		)
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)


	Adheasion ( 0.6 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 240kN )
	DerailBufferForce ( 400kN )
	WheelRadius ( 0.425m )
	NumWheels ( 5 )
	Friction (
		200N/m/s			1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s		0		1
	)
	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 100kN )

	MaxHandbrakeForce( 90kN )
	NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 15 )
	MaxApplicationRate( 15 )
	MaxAuxilaryChargingRate( 15 )
      BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

	Inside (
                  
			PassengerCabinFile ( DR_52_1331.s )
			PassengerCabinHeadPos ( -1.7 3.3 -5.8 )
			RotationLimit ( 0 180 0 )
			StartDirection ( 0 0 0 )
		)



	Lights	( 7
		Light	(
			Type( 1 )
			Conditions(
				Headlight ( 4 )
				Unit	( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	( 1
				State	(
					LightColour ( bbf8fc88 )
					Position ( 0.0 3.5 5 )
					Radius ( 50.0 )
					Angle ( 15.0 )
					)
				)
			)
		Light (
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					LightColour ( bbf8fc88 )
					Position ( 0 3.62 5.73 )
					Azimuth ( 0 0 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(	
			Type( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	( 1
				State	(
					LightColour ( bbf8fc88 )
					Position ( -0.872 1.48 6.32 )
					Azimuth ( 0 0 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light	(	
			Type( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	( 1
				State	(
					LightColour ( bbf8fc88 )
					Position ( 0.872 1.48 6.32 )
					Azimuth ( 0 0 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light (
			Type ( 0 )
			Conditions (
				TimeOfDay ( 2 )
				Service ( 2 )
				Control ( 1 )
				Unit ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					LightColour ( bbf8fc88 )
					Position ( 0 3.62 5.73 )
					Azimuth ( 0 0 0 )
					Radius ( 0.5 )
				)
			)
		)	
		Light	(	
			Type( 0 )
			Conditions (
				TimeOfDay ( 2 )
				Service ( 2 )
				Control ( 1 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	( 1
				State	(
					LightColour ( bbf8fc88 )
					Position ( 0.872 1.48 6.32 )
					Azimuth ( 0 0 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light	(	
			Type( 0 )
			Conditions (
				TimeOfDay ( 2 )
				Service ( 2 )
				Control ( 1 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	( 1
				State	(
					LightColour ( bbf8fc88 )
					Position ( -0.872 1.48 6.32 )
					Azimuth ( 0 0 0 )
					Radius ( 0.5 )			
					)
				)
			)
		)


	Sound ( "..//..//common.snd//Dampf_Sound//Lok_1400_DT.sms" )
	
	)


	Engine ( DR_52_1331_DT

	Effects
	(
		SteamSpecialEffects
		(
			comment
			(
				the format of these little blocks is as follow:

				offset.x offset.y offset.z
				normal.x normal.y normal.z
				width in metres

				defining the offset from the shape pivot point
				where steam / smoke should appear, the direction
				it should go and the width of the nozzle
			)

			WhistleFX
			(
				0.489 4.15 -4.748
				0 1 0
				0.05
			)

			SafetyValvesFX
			(
				0 4.11 -2.683
				0 1 0
				0.2
			)

			StackFX
			(
				0 4.4 4.05
				0 1 0
				0.2
			)

			DrainpipeFX
			(
				-1.5 1.258 -4.899
				-0.4 -1 -0.2
				0.05
			)

			CylindersFX
			(
				-1.1 0.4 3.757
				0 0 -1
				0.4
			)

			CylindersFX
			(
				1.1 0.4 3.757
				0 0 -1
				0.4
			)
		)
	)

	Wagon ( DR_52_1331_DT )
	Type ( Steam )
	MaxPower ( 1190kW )
	MaxForce ( 130kN )
	MaxVelocity ( 80kmh )
	IsTenderRequired( 1 )
	WheelRadius ( 0.70m )
	Sanding ( 1e9mph )
	NumWheels ( 5 )
	BoilerLength ( 6.0m )
	BoilerVolume ( "170*(ft^3)" )
	BoilerEffectivity ( 1.2 )
	DraftingEffect ( 0.7 )
	BoilerResponsiveness ( 1.1 )
	CoalBurnage ( 3.1lb/hp/h )
	MaxBoilerOutput ( 26000lb/h )
	NumCylinders ( 2 )
	CylinderStroke ( 66cm )
	CylinderDiameter ( 60cm )
	CylinderVolume ( "10.17*(ft^3)" )
	CylinderEffectivity ( 3.5 )
	InjectorSizes ( 12mm 12mm )
	ExhaustLimit ( 26000lb/h )
	PrimingFactor ( 1 )
	BlastExponent ( 0.95 )
	MaxBoilerPressure ( 228psi )
	MaxFireMass ( 3500lb )
	IdealFireMass ( 2500lb )
	MaxWaterMass ( 4200lb )
	SafetyValvesSteamUsage ( 25000lb/h )
	ShovelCoalMass ( 6lb )
	SmokeCombustion ( 1 )
	SteamSmokeUnitsPerPoundOfFuel( 5.5 )
	MaxTenderCoalMass ( 18000lb )
	MaxTenderWaterMass ( 50000lb )
	comment( 0 for live steam, 1 for exhaust steam )
	InjectorTypes( 0 0 )
	SuperHeater ( 1.25 )
	SteamGaugeGlassHeight( 11 )
	
	MaxSteamHeatingPressure( 60 )
	SafetyValvePressureDifference( 5 )

	BasicSteamUsage ( 750lb/h )
	BasicCoalUsage ( 310lb/h )
	InjectorLimits1 ( 50psi 0.5 1 )  
	InjectorLimits2 ( 50psi 0.5 1 )  
	CylinderCocksPowerEfficiency ( 0.85 )
	
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerMaxApplicationRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 35 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 72.5 )

	EngineBrakesControllerHasProportionalBrake( 1 )
      EngineBrakesProportionalBrakeLag( 0.9 )
        
      TrainBrakesControllerMaxPressureDropInNormalApplication( 70 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
      BrakesEngineControllers( "Hand, Train, Independent" )

	SteamCylinderCocksOperation( Manual )
	SteamSmallestCutoff( 0.08 )
	NumberOfDamperSteps( 4 )

	RegulatorValveType( Twin_port )
	RegulatorSecondValveStartPosition( 0.45 )
	RegulatorPilotValveExponent( 1.7 )
	RegulatorSecondValveExponent( 1.7 )
	RegulatorPilotValveFullOpenning( 0.35 )
	RegulatorMainValveInitialOpenning( 0.475 )

	SteamBlowerEffectExponent( 0.9 )
	SteamBlowerEfficiencyExponent( 1.1 )
	comment( lbs/h )
	SteamBlowerMaxSteamUsageRate( 500 )
	SteamBlowerMaxProportionOfBlastEffect( 0.15 )

    	AirBrakesAirCompressorPowerRating( 3 )
    	AirBrakesMainMinResAirPressure( 0 )
    	AirBrakesMainMaxAirPressure( 100 )
	AirBrakesMainResVolume( 8 )
    	AirBrakesCompressorRestartPressure( 95 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.25 )

    	EngineBrakesControllerHasProportionalBrake( 1 )

	TrainBrakesControllerMaxApplicationRate( 5 )
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 10 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 72.5 )

	EngineBrakesControllerMaxApplicationRate( 6 )
	EngineBrakesControllerMaxReleaseRate( 6 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72.5 )

	Sound ( "..//..//common.snd//Dampf_Sound//Lok_1_Cab.sms" )
	CabView ( PFT-TSP_26101.cvf )
	HeadOut ( 1.65 3.3 -5.7 )


      EngineControllers (
            Regulator ( 0 1 0.025 0 
                NumNotches( 0 )
            )
            Cutoff    ( -0.85 0.85 0.01 0 
                NumNotches( 0 )
            )
            Brake_Engine ( 0 1 0.02 0 
	            		NumNotches( 5
				Notch(0	0 	EngineBrakesControllerFullQuickReleaseStart )
    				Notch(0.1 	0 EngineBrakesControllerNeutralhandleOffStart) 
				Notch(0.2	1 EngineBrakesControllerApplyStart )
    				Notch(0.9 	0 EngineBrakesControllerFullServiceStart ) 
            				Notch(1.0 	0 EngineBrakesControllerEmergencyStart ) 
            			)
		)

           		Brake_Train ( 0 1 0.02 0.3 
	            		NumNotches( 5
				Notch(0		0 TrainBrakesControllerReleaseStart )
    				Notch(0.1 	0 TrainBrakesControllerNeutralhandleOffStart)
				Notch(0.2	1 TrainBrakesControllerApplyStart ) 
    				Notch(0.9 	0 TrainBrakesControllerFullServiceStart ) 
            				Notch(1.0 	0 TrainBrakesControllerEmergencyStart )
	            		)
		)


            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            FireDoor ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Sanding( 0 1 0 )
            Blower ( 0 1 0.025 0.2 
                NumNotches( 0 )
            )
            HeatingTap ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Shovel ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            DampersFront ( 0 1 0.1 1
                NumNotches( 0 )
            )
            DampersBack ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector1Steam ( 0 1 0 )
            Injector2Steam ( 0 1 0 )
            Injector1Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector2Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            CylinderCocks ( 0 1 1 )
            Whistle ( 0 1 0 )
            SmallEjectorOrCompressor( 0 1 1 )
            BellToggle( 0 1 0 )
            Headlights( 0 1 0 )
        )
	comment(fire temp, fire mass, water mass, boiler pressure,
		tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )
	EngineVariables( 970 1950 1850 180 50000 18000 350 1 1 )
	
	Name ( "DR_52_1331_DT_Bw_Angermünde" )


	Description (
	"IdealFireMass pro budovatelskou smes: 1836lb - nastaveno \n\n"+
	"Lokomotiva rady 555.0 \n"+
	"Charakteristiky:\n"+
	"Rok vyroby: 1942 - 1945 \n"+
	"Pocet vyrobenych kusu: cca. 6600\n"+
	"Posledni vyrazena: \n"+
	"Usporadani: dvojcita (dvouvalcova), usp. naprav 1' E \n"+
	"Prumer kol: 1400 mm\n"+
	"Pretlak pary v kotli: 1600 atm\n"+
	"Max. vykon: 1216 kW\n"+
	"Vaha loko ve sluzbe: 84.3 t\n"+
	"Kluzna napravova loziska\n"+
	"Prumer valcu 600 mm\n"+
	"Max. rychl.: 80 km/h\n"	
	
	)


	EngineOperatingProcedures (

     	"Jak se rozjet\n"+
      "1. Nastav kolo rozvodu [W] lokomotivy plne vylozeni.\n"
	"2. Stiskni a drz [;] pro uvolneni vlakove brzy.\n"+
      "2a. Stiskni a drz [[] -leva hranata zavorka- na uvolneni lokomotivni brzdy.\n"+	
      "3. Stiskni a drz regulator pary [D] pro zvyseni tlaku pary ve valcich.\n"+  
	"4. Kdyz se lokomotiva zacne rozjizdet, stiskni a drz regulator rozvodu [S] a snizuj postupne vylozeni po 10 stupnich, az ma lokomotiva potrebnou rychlost.\n\n"+
	"Jak zpomalit vlak\n"+
	"1. Stiskni a drz regulátor rozvodu [S] a sniz tak jeho vylozeni.\n"+
	"2. Nestaci. Pak stiskni a drz regulator pary [A] pro snizeni taku pary ve valcich.\n"+
	"Poznamky:\n\n"
	"Pro optimalni jizdu by mel byt regulator pary nastaven na co nejvyssi hodnotu a rychlost by se mela prednostne regulovat prestavovanim rozvodu. Tehdy pracuje kotel a parni stroj s optimalní ucinnosti.\n\n"+
	"Hodnoty regulatoru rozvodu 0 az max jsou pro jizdu vpred, hodnoty 0 az -max pro jizdu vzad.\n\n"
	"Brzdeni vlakovou brzdou\n"+
	"1. Stiskni a drz ['] pro brzdeni vlakovou brzdou.\n"+
	"2. Az dosahnes potrebne brzdne sily, presun stisknutim [;] brzdic do neutralni polohy.\n\n"+
	"Uvolneni vlakove brzdy\n"+
	"1. Stiskni a drz [;] pro odbrzdeni vlakove brzdy.\n"+
	"2. Po odbrzdeni vlakove brzdy presun stisknutim ['] brzdic do neutralni polohy.\n\n"+
	"Jízda dozadu\n"+
	"1. Zastav vlak.\n"+ 
      "2. Stiskni regulátor rozvodu [S] a drz, dokud se neprestavi rozvod lokomotivy na plne vylozeni 'vzad'.\n"
	"3. Stiskni a drz [;] pro uvolneni vlakove brzy.\n"+
      "3a. Stiskni a drz [[] -leva hranata zavorka- na uvolneni lokomotivni brzdy.\n"+	
      "4. Stiskni a drz regulator pary [D] pro zvyseni tlaku pary ve valcich.\n"+  
	"5. Kdyz se lokomotiva zacne rozjizdet, stiskni a drz regulator rozvodu [W] a pomalu sniz vylozeni, az ma lokomotiva potrebnou rychlost.\n\n"+
	"Nastup a vystup cestujicich\n"+
	"1. Zastav ve stanici.\n"+
	"2. Stiskni [ENTER].\n"+
	"3. Vyckej "Rozkazu k odjezdu".\n"+

	"Jak pripojit dalsi vozidla\n"+
	"1. Velmi pomalu najed na soupravu.\n"+
	"TIP: Nejlepsi pohled pro pripojeni soupravy je pod [6].\n"+
	"2. Zmackni [F9] pro otevreni okna sestavy vlaku.\n"+
	"3. Pokud je ikona nektereho z pripojovanych vozu cervena, ma tento vuz zatazenou rucni brzdu. Tukni 2x mysi na ikonu vozu pro uvolneni rucni brzdy.\n"+
	"4. Zavri okno sestavy vlaku ([F9] nebo mysi na [X]).\n\n"+
	"Jak odpojit cast vlaku\n"+
	"POZOR! Melo by se provadet jen tehdy, pokud VLAK STOJI!\n"
	"1. Otevri okno sestavy vlaku [F9].\n"+
	"2. Pokud chces zatahnout rucni brzdu na odstavovanem voze, klepni 2x mysi na jeho ikonu. Ikona zcervena.\n"+
	"3. Klepni 2x mysi na symbol sprahla v miste, kde ma byt vlak rozdelen.\n"+
	"4. Zavri okno sestavy vlaku ([F9] nebo mysi na [X]).\n\n"
	)
)





