SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( DR_86_1053
	Type ( Engine )
	WagonShape ( DR_86_1053.s )
	FreightAnim ( DR_86_1053_Details.s 1 1 )
	Size  ( 3.05m 4.22m 13.5m )
	CentreOfGravity ( 0m 1.7m 0m )
	Centre ( 0m 0m 0m )
	Mass ( 88.5t )
	InertiaTensor ( Box(3.05m 4.22m 13.5m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 4e6N/m 5e6N/m )
			Damping ( 3e6N/m/s 3e6N/m/s )
			Break ( 9.5e7N 9.5e7N )
			r0 ( 20cm 30cm )
		)
		Velocity ( 0.1m/s )
	)

	Adheasion ( 0.15 0.3 2 0.0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 210kN )
	DerailBufferForce ( 800kN )
	WheelRadius ( 0.425m )
	NumWheels ( 1 )
	Friction (
		1312N/m/s		1	      1mph		      16.33N/m/s		1.8
		5.1N/rad/s		1		-1rad/s		0		1
	)
	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 80kN )

	MaxHandbrakeForce( 90kN )
	NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 25 )
	MaxApplicationRate( 25 )
	MaxAuxilaryChargingRate( 95 )
      BrakeCylinderPressureForMaxBrakeBrakeForce( 60 )

      Inside (
		PassengerCabinFile ( DR_86_1053.s )
		PassengerCabinHeadPos ( -1.5 3.3 -3.45 )
		RotationLimit ( 90 360 0 )
		StartDirection ( 0 0 0 )
	)

	IntakePoint ( -1.2 2.0 FuelWater )
	IntakePoint ( -5.3 2. FuelCoal )


	Lights	( 8
		Light	(
			comment( Sphere of light )
			Type( 1 )
			Conditions(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffd5 )
					Position ( 0.0 3 6 )
					Transition ( 0 )
					Radius ( 50.0 )
					Angle ( 15.0 )
					)
				)
			)
           Light	(
			comment( Feuerschein )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Unit ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	3
				State	(
					Duration ( 0.05 )
					LightColour ( 80ff7200 )
					Position ( 0 2.3 -3.325 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.4 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( 80ffe610 )
					Position ( 0 2.3 -3.325 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.4 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( 80ff7830 )
					Position ( 0 2.3 -3.325 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.4 )
					)
				)
			)
		Light	(	
			comment( Head light right dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control (0)
				Service (0)
				TimeOfDay (0)
				Weather (0)
				Coupling (0)
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -0.842 1.5 6.228 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.6 )
					)
				)
			)
		Light	(
			comment( Head light left dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control (0)
				Service (0)
				TimeOfDay (0)
				Weather (0)
				Coupling (0)
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 0.842 1.5 6.228 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.6 )
					)
				)
			)
			Light	(
			comment( Head light top dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control (0)
				Service (0)
				TimeOfDay (0)
				Weather (0)
				Coupling (0)
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 0 3.22 5.825 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
			Light	(	
			comment( Head light right dim back)
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Control (0)
				Service (0)
				TimeOfDay (0)
				Weather (0)
				Coupling (0)
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -0.842 1.5 -6.283 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
					)
				)
			)
		Light	(
			comment( Head light left dim back)
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Control (0)
				Service (0)
				TimeOfDay (0)
				Weather (0)
				Coupling (0)
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 0.842 1.5 -6.283 )
					Azimuth (  -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
					)
				)
			)
			Light	(
			comment( Head light top dim back)
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Control (0)
				Service (0)
				TimeOfDay (0)
				Weather (0)
				Coupling (0)
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 0 3.645 -6.24 )
					Azimuth (  -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
	)
	Sound ( "BR86eng.sms" )

)

Engine ( DR_86_1053
	Effects
	(
		SteamSpecialEffects
		(
			comment
			(
				the format of these little blocks is as follow:

				offset.x offset.y offset.z
				normal.x normal.y normal.z
				width in metres

				defining the offset from the shape pivot point
				where steam / smoke should appear, the direction
				it should go and the width of the nozzle
			)

			WhistleFX
			(
				0.476 3.83 0.495
				0 1 0
				0.25
			)

			SafetyValvesFX
			(
				0 3.9 -0.33
				0 1 0
				0.2
			)

			StackFX
			(
				0 4.12 4.1
				0 1 0
				0.225
			)

			DrainpipeFX
			(
				-1.5 1.258 -4.899
				-0.4 -1 -0.2
				0.05
			)

			CylindersFX
			(
				-1.12 0.65 4.12
				0 -1 0
				0.175
			)

			CylindersFX
			(
				1.12 0.65 4.12
				0 -1 0
				0.175
			)
		)
	)

	Wagon ( DR_86_1053 )
      IsTenderRequired( -1 )	
	Type ( Steam )
	MaxPower ( 775kW )
	MaxForce ( 110kN )
     	MaxVelocity ( 80kmh )
	WheelRadius ( 0.70m )
	NumWheels ( 4 )
	Sanding ( 1e25kmh )
 
      BoilerLength ( 4.5m )
	BoilerVolume ( "6.3*(m^3)" )
	BoilerEffectivity ( 1.26 )
	DraftingEffect ( 0.9 )
	BoilerResponsiveness ( 1.2 )
	CoalBurnage ( 4.0lb/hp/h )
	MaxBoilerOutput ( 22500lb/h )
                 
	NumCylinders ( 2 )
	CylinderStroke ( 66cm )
	CylinderDiameter ( 57cm )
	CylinderVolume ( "376200*(cm^3)" )
	CylinderEffectivity ( 1.2 )
	CylinderCocksPowerEfficiency ( 0.8 )
	SteamCylinderCocksOperation( Manual )

      ExhaustLimit ( 24000lb/h )
	PrimingFactor ( 1 )
	BlastExponent ( 0.7 )
	MaxBoilerPressure ( 14bar )
	SuperHeater ( 1.2 )
	MaxFireMass ( 1700lb )
	IdealFireMass ( 1100lb )
	MaxWaterMass ( 3500lb )  

      ShovelCoalMass ( 18lb )
	SmokeCombustion ( 1 )
	
	MaxTenderCoalMass ( 8828lb )
	MaxTenderWaterMass ( 19863lb )

      SteamSmokeUnitsPerPoundOfFuel( 2 )
	SteamMaxSmokeUnitsReleaseRate( 25 )
	SteamSmokeUnitsPerPoundOfFuel( 6.3 )

	SafetyValvesSteamUsage ( 9000lb/h )
	SafetyValvePressureDifference( 1.05 )
	SteamGaugeGlassHeight( 11 )

	SteamSmallestCutoff( 3 )
      NumberOfDamperSteps( 4 )

	BasicSteamUsage ( 2400lb/h )
	BasicCoalUsage ( 500lb/h )
 
                InjectorSizes ( 10mm 10mm )
	InjectorTypes( 0 1 ) 
	InjectorLimits1 ( 30psi 0.3 1 )
	InjectorLimits2 ( 30psi 0.3 1 )
		
	
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 116 )
	AirBrakesMainResVolume( 28 )
	AirBrakesCompressorRestartPressure( 116 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 3.0 )

	TrainBrakesControllerMinPressureReduction( 1 )
	TrainBrakesControllerMaxApplicationRate( 10 )
	TrainBrakesControllerMaxQuickReleaseRate ( 50 )
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 73 )
	TrainBrakesControllerFullServicePressureDrop( 22 )
	TrainBrakesControllerEmergencyApplicationRate( 22 )

	EngineBrakesControllerMinPressureReduction( 1 )
	EngineBrakesControllerMaxApplicationRate( 5 )
	EngineBrakesControllerMaxQuickReleaseRate ( 50 )
	EngineBrakesControllerMaxReleaseRate( 5 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 73 )
	EngineBrakesControllerFullServicePressureDrop( 22 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
      BrakesEngineControllers( "Independent, Train" )


      SteamSmallestCutoff( 3 )
      NumberOfDamperSteps( 4 )

	RegulatorValveType( Twin_port )
	RegulatorSecondValveStartPosition( 0.45 )
	RegulatorPilotValveExponent( 1.47 )
	RegulatorSecondValveExponent( 1.8 )
	RegulatorPilotValveFullOpenning( 0.45 )
	RegulatorMainValveInitialOpenning( 0.475 )
 
      SteamBlowerEffectExponent( 0.5 )
	SteamBlowerEfficiencyExponent( 1.1 )
	comment( lbs/h )
	SteamBlowerMaxSteamUsageRate( 500 )
	SteamBlowerMaxProportionOfBlastEffect( 0.25 )

      CabView ( BR86.cvf )
	HeadOut ( 1.65 3.3 -3.7 )

        EngineControllers (
            Regulator ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            Cutoff    ( -0.85 0.85 0.02 0 
                NumNotches( 0 )
            )
            Brake_Engine ( 0 1 0.02 0 
	            NumNotches( 5
					Notch(0	0 EngineBrakesControllerFullQuickReleaseStart )
    					Notch(0.1 	0 EngineBrakesControllerNeutralhandleOffStart) 
					Notch(0.2	1 EngineBrakesControllerApplyStart )
    					Notch(0.9 	0 EngineBrakesControllerFullServiceStart ) 
            			Notch(1.0 	0 EngineBrakesControllerEmergencyStart ) 
            			)
		)

           	Brake_Train ( 0 1 0.02 0.3 
	            NumNotches( 5
					Notch(0	0 TrainBrakesControllerReleaseStart )
    					Notch(0.1 	0 TrainBrakesControllerNeutralhandleOffStart)
					Notch(0.2	1 TrainBrakesControllerApplyStart ) 
    					Notch(0.9 	0 TrainBrakesControllerFullServiceStart ) 
            			Notch(1.0 	0 TrainBrakesControllerEmergencyStart )
	            		)
		)

            FireDoor ( 0 1 1 0 
                NumNotches( 0 )
            )
            Sanding( 0 1 0 )
            Blower ( 0 1 0.025 0.2 
                NumNotches( 0 )
            )
            HeatingTap ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Shovel ( 0 1 1 0 
                NumNotches( 0 )
            )
            DampersFront ( 0 1 0.1 1
                NumNotches( 0 )
            )
            DampersBack ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector1Steam ( 0 1 0 )
            Injector2Steam ( 0 1 0 )
            Injector1Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector2Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            CylinderCocks ( 0 1 1 )
            Whistle ( 0 1 0 )
            SmallEjectorOrCompressor( 0 1 1 )
            BellToggle( 0 1 0 )
            Headlights( 0 1 0 )
        )
	comment(fire temp, fire mass, water mass, boiler pressure,
		tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )

	EngineVariables( 890 1000 3750 180 19863 8828 250 1 1 )

	Sound ( "BR86cab.sms" )
	Name ( "DR_86_1053_Bw_Zittau" )

	Description (
	"Dampflok der BR 86 der DR\n\n"+
	"Lokomotivtyp: 1´D1´-h2t \n\n"+
      "1.Baujahr: 1928 \n\n"+
	"Maximaler Dampfkesseldruck: 14 bar \n\n"+
	"Höchstgeschwindigkeit (zulässig): 80 km/h (bis 86 234 =70km/h) \n\n"+
	"Gewicht: 88,5t\n\n"+
      "Achslast max: 15,6t\n\n"+
	"Fassungsvermögen Kohle: 4,0 Tonnen \n\n"+
	"Fassungsvermögen Wasser: 9.000 Liter \n\n"+
	"Bremsen: Luft\n\n"
	)
	EngineOperatingProcedures (
	"So setzen Sie den Zug in Bewegung\n"+
	"1.	Drücken Sie mehrmals die W-TASTE, um den Richtungshebel ganz auf Vorwärts zu stellen.\n"+
	"2.	Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n"+
	"3.	Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n"+
	"4.	Drücken Sie die D-TASTE, um den Regler zu erhöhen.\n"+  
	"5.	Drücken Sie während des Beschleunigens die S-TASTE, um den Regler langsam zurückzunehmen. Stellen Sie den Regler dann so ein, dass die gewünschte Geschwindigkeit beibehalten wird.\n\n"+ 
	"So bremsen Sie den Zug ab\n"+
	"1.	Drücken Sie die A-TASTE, um den Regler in eine niedrigere Position zu stellen.\n"+
	"2.	Setzen Sie die Bremsen ein, wenn Sie noch weiter abbremsen möchten.\n\n"+   
	"So bedienen Sie die Zugbremsen\n"+
	"1.	Drücken Sie die Ä-TASTE, um die Zugbremse zu ziehen.\n\n"+
	"So lösen Sie die Zugbremsen\n"+
	"1. Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n\n"+
	"So betätigen Sie die Lokbremse\n"+
	"1.	Drücken Sie die +-TASTE (Pluszeichen), um die Lokbremse anzuziehen.\n\n"+
	"So lösen Sie die Lokbremse\n"+
	"1. Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n\n"+
	"So fahren Sie rückwärts\n"+
	"1.	Halten Sie den Zug vollständig an.\n"+
	"2.	Drücken Sie mehrmals die S-TASTE, um den Richtungshebel ganz auf Rückwärts zu stellen.\n"+
	"3.	Drücken Sie die Ö-TASTE, um die Bremsen zu lösen.\n"+
	"4.	Schieben Sie den Regler langsam nach vorne (D-TASTE).\n\n"+
	"So lassen Sie Fahrgäste ein- und aussteigen\n"+
	"1. Halten Sie an einem Bahnhof an.\n"+
	"2. Drücken Sie die EINGABETASTE.\n"+
	"3. Warten Sie auf die \"permission to depart\" Signalpfeife.\n"+
	"TIPP: Verwenden Sie die Lokführerinformation 'Nächster Halt' (F10), um das Ein- und Aussteigen zu überwachen.\n\n"+
	"So kuppeln Sie an einen Waggon oder eine Lokomotive an\n"+
	"1. Fahren Sie sehr langsam an die Einheit heran, mit etwa 4 km/h.\n"+
	"TIPP: Drücken Sie die 6-TASTE, um in die Kupplungsansicht zu wechseln.\n"+
	"2. Drücken Sie F9, um das Zugbedienungsfenster zu öffnen.\n"+
	"3. Wenn das Symbol für die angekuppelte Einheit rot angezeigt wird, ist die Handbremse gezogen. Doppelklicken Sie auf den Waggon, um die Handbremse zu lösen.\n"+
	"4. Schließen Sie das Zugbedienungsfenster.\n\n"+
	"So kuppeln Sie von einem Waggon oder einer Lokomotive ab\n"+
	"1. Drücken Sie F9, um das Zugbedienungsfenster zu öffnen.\n"+
	"2. Doppelklicken Sie auf eine Einheit in dem Bereich des Zuges, den Sie von der Lokomotive abkuppeln möchten, um die Handbremse zu ziehen.\n"+
	"3. Doppelklicken Sie auf die Kupplung zwischen den Einheiten, die Sie vom Rest des Zuges abkuppeln möchten.\n"+
	"4. Klicken Sie auf die grüne 'Kupplung' zwischen den Einheiten, die Sie abkuppeln möchten.\n"+
	"5. Klicken Sie auf die Schaltfläche 'Abkuppeln'.\n"+
	"6. Schließen Sie das Zugbedienungsfenster.\n\n"+
	"Befehle zum Befeuern (Computergesteuerter Heizer 'Aus' auf dem Bildschirm 'Optionen')\n"+
	"So füllen Sie Kohle in die Feuerbüchse nach\n"+
	"1. Drücken Sie die F-TASTE, um die Feuertür zu öffnen.\n"+
	"2. Drücken Sie die R-TASTE, um die Schaufelrate zu erhöhen.\n\n"+
	"So beenden Sie das Hinzufügen von Kohle\n"+
	"1. Drücken Sie UMSCHALT+R, um die Schaufelrate zu verringern.\n"+
	"2. Drücken Sie UMSCHALT+F, um die Feuertür zu schließen.\n"+
	"So bedienen Sie den Hilfsbläser\n\n"+
	"1.	Drücken Sie die N-TASTE, um den Hilfsbläser zu verstärken.\n"+
	"2. Drücken Sie UMSCHALT+N, um den Hilfsbläser zu drosseln.\n\n"+
	"So bedienen Sie die Luftklappen\n"+
	"1.	Drücken Sie die M-TASTE, um die Luftklappen zu öffnen.\n"+
	"2. Drücken Sie UMSCHALT+M, um die Luftklappen zu schließen.\n\n"+
	"So spritzen Sie Wasser in den Dampfkessel ein\n"+
	"1.	Drücken die I-TASTE, um den Dampf für Dampfstrahlpumpe 1 einzuschalten.\n"+
	"(Sie können auch die O-TASTE drücken, um den Dampf für die Dampfstrahlpumpe 2 einzuschalten.)\n"+
	"2.	Drücken Sie die K-TASTE, um die Wasserzufuhr für die Dampfstrahlpumpe 1 zu erhöhen.\n"+
	"(Drücken Sie die L-TASTE, um die Wasserzufuhr für die Dampfstrahlpumpe 2 zu erhöhen.)\n\n"+
	"So schalten Sie die Wassereinspritzung in den Dampfkessel ab\n"+
	"1. Drücken Sie die I-TASTE, um den Dampf für die Dampfstrahlpumpe 1 auszuschalten.\n"+
	"2. Drücken Sie die O-TASTE, um den Dampf für die Dampfstrahlpumpe 2 abzuschalten."
	)
)

