SIMISA@@@@@@@@@@JINX0h0t______

Tr_CabViewFile (
	CabViewType ( 2 )
	CabViewFile ( front.ace )
	CabViewWindow ( 0 0 640 480 )
	CabViewWindowFile ( AcWndFrn.ace )
	Position ( 0.75 3.5 6 )
	Direction ( 10 2 0 )
	CabViewFile ( links.ace )
	CabViewWindow ( 0 0 640 480 )
	CabViewWindowFile ( AcWndLft.ace )
	Position ( 0.75 3.5 6 )
	Direction ( 5 -42 0 )
	CabViewFile ( rechts.ace )
	CabViewWindow ( 0 0 640 480 )
	CabViewWindowFile ( AcWndRgt.ace )
	Position ( 0.75 3.5 6 )
	Direction ( 8 68 0 )
	EngineData ( GP38 )
	CabViewControls ( 11
		TriState (
			Type ( DIRECTION TRI_STATE )
			Position ( 45 360 69 62 )
			Graphic ( fahrtw.ace )
			NumFrames ( 3 1 3 )
			Style ( NONE )
			MouseControl ( 1 )
			Orientation ( 0 )
			DirIncrease ( 0 )
		)
		Lever (
			Type ( THROTTLE LEVER )
			Position ( 89 312 209 114 )
			Graphic ( fahrsch.ace )
			Style ( NOT_SPRUNG )
			MouseControl ( 1 )
			NumFrames ( 6 2 3 )
			NumPositions ( 0 )
			NumValues ( 0 )
			Orientation ( 0 )
			DirIncrease ( 0 )
			ScaleRange ( 0 1 )
		)
		Lever (
			Type ( ENGINE_BRAKE LEVER )
			Position ( 414 207 115 41 )
			Graphic ( lbv.ace )
			Style ( NOT_SPRUNG )
			MouseControl ( 1 )
			NumFrames ( 3 1 3 )
			NumPositions ( 1 0 )
			NumValues ( 1 0 )
			Orientation ( 0 )
			DirIncrease ( 0 )
			ScaleRange ( 0 1 )
		)
		TriState (
			Type ( FRONT_HLIGHT TRI_STATE )
			Position ( 332 414 84 32 )
			Graphic ( licht.ace )
			NumFrames ( 3 1 3 )
			Style ( NONE )
			MouseControl ( 1 )
			Orientation ( 0 )
			DirIncrease ( 0 )
		)
		TwoState (
			Type ( SANDERS TWO_STATE )
			Position ( 428 412 14 29 )
			Graphic ( sand.ace )
			NumFrames ( 2 2 1 )
			Style ( ONOFF )
			MouseControl ( 1 )
		)
		TwoState (
			Type ( RESET TWO_STATE )
			Position ( 57 448 37 30 )
			Graphic ( sifataster.ace )
			NumFrames ( 2 1 2 )
			Style ( PRESSED )
			MouseControl ( 1 )
		)
		Digital (
			Type ( SPEEDOMETER DIGITAL )
			Position ( 368 329 32 32 )
			ScaleRange ( 0 150 )
			Accuracy ( 0 )
			AccuracySwitch ( 0 )
			LeadingZeros ( 0 )
			Justification ( 3 )
			PositiveColour ( 0
				ControlColour ( 0 0 0 )
			)
			NegativeColour ( 0 )
			DecreaseColour ( 0 )
			Units ( KM_PER_HOUR )
		)
		MultiStateDisplay (
			Type ( ALERTER_DISPLAY MULTI_STATE_DISPLAY )
			Position ( 318 340 19 15 )
			Graphic ( lm_sifa.ace )
			States ( 2 1 2
				State (
					Style ( 0 )
					SwitchVal ( 0 )
				)
				State (
					Style ( 0 )
					SwitchVal ( 1 )
				)
			)
		)
		Gauge (
			Type ( EQ_RES GAUGE )
			Position ( 489 327 10 28 )
			Area ( 0 0 8 2 )
			Graphic ( nadel.ace )
			Style ( POINTER )
			ScaleRange ( 0 10 )
			ZeroPos ( 0 )
			PositiveColour ( 1
				ControlColour ( 0 0 0 )
			)
			NegativeColour ( 0 )
			Orientation ( 1 )
			DirIncrease ( 1 )
			Units ( BAR )
		)
		Gauge (
			Type ( BRAKE_CYL GAUGE )
			Position ( 455 330 8 30 )
			Area ( 0 0 8 2 )
			Graphic ( nadel.ace )
			Style ( POINTER )
			ScaleRange ( 0 10 )
			ZeroPos ( 0 )
			PositiveColour ( 1
				ControlColour ( 0 0 0 )
			)
			NegativeColour ( 0 )
			Orientation ( 1 )
			DirIncrease ( 1 )
			Units ( BAR )
		)
		Lever (
			Type ( TRAIN_BRAKE LEVER )
			Position ( 427 323 132 65 )
			Graphic ( fbv.ace )
			Style ( NOT_SPRUNG )
			MouseControl ( 1 )
			NumFrames ( 6 2 3 )
			NumPositions ( 5 0 1 3 4 5 )
			NumValues ( 5 0 0.3 0.85 0.9 0.95 )
			Orientation ( 0 )
			DirIncrease ( 0 )
			ScaleRange ( 0 1 )
		)
	)
)