ČD Class AB Passenger Carriage for MSTS - Full Version 3.0
------------------------------------------------------------------------------------
Produced 1984, Goerlitz Va bogies

3D model, textures, wag files: Ondra Janiš
Carriage body basic 3D model: Rado Rabatin (radorabatin@gmail.com)
Photo documentation: Thunderbird (thunderbird@email.cz), Ondra Janiš   

ATTENTION: This add-on is ONLY usable with MSTS BIN installed! More info at mstsbin.uktrainsim.com 

------------------------------------------- 
FREEWARE
Although this model/add-on is free, it still remains property of the author(s).
WITHOUT HIS (THEIR) PERMISSION IT IS NOT ALLOWED to distribute the archive or it's parts on the internet 
(with the only exception of sites chosen by the author(s)) or on CD, and in CANNOT BE IN ANY CASE SOLD or 
be part of any COMMERCIAL ADD-ON. Exceptions are defined by the author(s).

It is generally allowed to make repaints, but please let me know about it.
-------------------------------------------

ATTENTION:
 Coupling length is set to MSTS Default 30cm. In case that you use the 80cm coupling length in 
default.wag, please copy all files from the "80cm" subfolder to the basic folder of the car,
rewriting the original ones.

INSTALLATION:
	1. Unpack all files from the archive to the MSTS master directory (preserve the archive's folder structure)
	2. Use the existing consists or create one using the MSTS Consist Editor


Comments, questions: vdojanis@volny.cz
For further updates and new add-ons visit: http://ondraj-msts.ic.cz/
