SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RA-BD-BR143-N-D
	Type ( Engine )
	WagonShape ( "RA-BD-BR143-D.s" )
	Size ( 3.312m 4.762m 16.902m )
	Mass ( 82.5t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.312m 4.762m 16.902m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 4.8E6N/m 0N/m )
			Damping ( 1.1E6N/m/s 0N/m/s )
			Break ( 6E7N 6E7N )
			r0 ( 0m 1E9m )
		)
		CouplingHasRigidConnection (  )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1E7N/m 0N/m )
			Damping ( 1E6N/m/s 0N/m/s )
			r0 ( 0m 1E9m )
		)
		Centre ( 0.5m )
		Radius ( 1m )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.25 0.49 1.8 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 1290kN )
	DerailBufferForce ( 250kN )
	NumWheels ( 4 )
	Friction (
		1725N/m/s	0	0.7mph	19.45N/m/s	1.8
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)
	AntiSlip (  )
	BrakeEquipmentType ( "triple_valve,auxilary_reservoir,emergency_brake_reservoir" )
	BrakeSystemType ( Air_single_pipe )
	MaxBrakeForce ( 82.5kN )
	EmergencyBrakeResMaxPressure ( 145.038 )
	TripleValveRatio ( 2.5 )
	MaxReleaseRate ( 30 )
	MaxApplicationRate ( 25 )
	MaxAuxilaryChargingRate ( 20 )
	EmergencyResCapacity ( 10 )
	EmergencyResChargingRate ( 25 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 50.763 )
	Lights ( 17
		Light (
			comment ( Lichtkegel #1 )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFB6926D )
					Position ( 0 1.5 25 )
					Angle ( 20 )
					Transition ( 0 )
					Radius ( 150 )
				)
			)
		)
		Light (
			comment ( Lichtkegel #2 )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFAD09F )
					Position ( 0 1.5 25 )
					Angle ( 25 )
					Transition ( 0 )
					Radius ( 200 )
				)
			)
		)
		Light (
			comment ( vorn mitte abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFADEBD )
					Position ( 0 2.509 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( -4 -4 -4 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( vorn rechts abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFADEBD )
					Position ( -1.05 1.61 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( vorn links abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFADEBD )
					Position ( 1.05 1.61 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( vorn mitte aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( 0 2.509 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( -4 -4 -4 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( vorn rechts aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( -1.05 1.61 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( vorn links aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( 1.05 1.61 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( hinten rechts abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0 )
			FadeOut ( 0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.68 1.61 -7.9 )
					Azimuth ( 180 180 180 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( hinten links abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0 )
			FadeOut ( 0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.68 1.61 -7.9 )
					Azimuth ( 180 180 180 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( hinten rechts aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0 )
			FadeOut ( 0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.68 1.61 -7.9 )
					Azimuth ( 180 180 180 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.9 )
				)
			)
		)
		Light (
			comment ( hinten links aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0 )
			FadeOut ( 0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.68 1.61 -7.9 )
					Azimuth ( 180 180 180 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.9 )
				)
			)
		)
		Light (
			comment ( AI vorn mitte  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( 0 2.509 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( -4 -4 -4 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( AI vorn rechts  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( -1.05 1.61 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( AI vorn links  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( 1.05 1.61 7.9 )
					Azimuth ( 0 0 0 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( AI hinten rechts  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.68 1.61 -7.9 )
					Azimuth ( 180 180 180 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( AI hinten links  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.68 1.61 -7.9 )
					Azimuth ( 180 180 180 )
					Elevation ( 2.5 2.5 2.5 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
	)
	Sound ( "pt_143eng.sms" )
)

Engine ( RA-BD-BR143-N-D
	Wagon ( "RA-BD-BR143-N-D" )
	Type ( Electric )
	MaxPower ( 3700kW )
	MaxForce ( 128kN )
	MaxContinuousForce ( 240kN )
	MaxVelocity ( 117km/h )
	MaxCurrent ( 1640A )
	WheelRadius ( 0.5m )
	Sanding ( 1E9mph )
	NumWheels ( 3 )

	HeadOut ( 1.65m 3.166m 7.208m )

	AirBrakesAirCompressorPowerRating ( 1.2 )
	AirBrakesAirCompressorWattage ( 10000 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.22 )
	AirBrakesCompressorRestartPressure ( 120 )
	AirBrakesIsCompressorElectricOrMechanical ( 1 )
	AirBrakesMainMaxAirPressure ( 145.038 )
	AirBrakesMainMinResAirPressure ( 0 )
	AirBrakesMainResVolume ( 8 )
	EngineBrakesControllerMinPressureReduction ( 6 )
	EngineBrakesControllerMaxApplicationRate ( 20 )
	EngineBrakesControllerMaxReleaseRate ( 15 )
	EngineBrakesControllerEmergencyApplicationRate ( 50 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 72.52 )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	EngineBrakesControllerFullServicePressureDrop ( 26 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	TrainBrakesControllerMinPressureReduction ( 6 )
	TrainBrakesControllerMaxApplicationRate ( 20 )
	TrainBrakesControllerMaxReleaseRate ( 4 )
	TrainBrakesControllerEmergencyApplicationRate ( 50 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 72.52 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerFullServicePressureDrop ( 26 )
	EngineBrakesProportionalBrakeLag ( 0.9 )

	DynamicBrakesMinUsableSpeed ( 5 )
	DynamicBrakesMaximumEffectiveSpeed ( 5 )
	DynamicBrakesMaximumForce ( 150kN )
	DynamicBrakesResistorCurrentLimit ( 5000 )
	DynamicBrakesCutInSpeed ( -150 )
	DynamicBrakesMaxAirBrakePressure ( 70 )
	DynamicBrakesFadingSpeed ( 130 )
	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
	DynamicBrakesMaximumSpeedForFadeOut ( 140 )
	DynamicBrakesEffectAtMaximumFadeOut ( 0 )
	DynamicBrakesHigherSpeedCurveExponent ( 1 )
	DynamicBrakesLowerSpeedCurveExponent ( 1 )
	DynamicBrakesNumberOfControllerNotches ( 8 )
	BrakesEngineBrakeType ( Air_single_pipe )
	BrakesTrainBrakeType ( Air_single_pipe )
	BrakesEngineControllers ( "Train,Independent,Dynamic" )
	DoesBrakeCutPower ( 1 )

	CabView ( "nacht\\pt_143-N.cvf" )

	DoesHornTriggerBell ( 0 )

	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 45 )
		MonitoringDeviceAlarmTimeLimit ( 30 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
	)
	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnResetButton ( 1 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 300 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
		MonitoringDeviceResetOnResetButton ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
	)

	EngineControllers (
		AWS ( 0 1 0 )
		BailOffButton ( 0 1 0 )
		BellToggle ( 0 1 0 )
		Brake_Dynamic ( 0 1 0.11 0
			NumNotches ( 10
				Notch ( 0 0 Dummy )
				Notch ( 0.11 0 Dummy )
				Notch ( 0.22 0 Dummy )
				Notch ( 0.33 0 Dummy )
				Notch ( 0.44 0 Dummy )
				Notch ( 0.55 0 Dummy )
				Notch ( 0.66 0 Dummy )
				Notch ( 0.77 0 Dummy )
				Notch ( 0.88 0 Dummy )
				Notch ( 1 0 Dummy )
			)
		)
		Brake_Engine ( 0 1 0.025 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Train ( 0 1 0.0125 0.28
			NumNotches ( 6
				Notch ( 0 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.2 0 TrainBrakesControllerHoldLappedStart )
				Notch ( 0.25 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.85 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.9 0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
			)
		)
		Throttle ( 0 1 0.025 0
			NumNotches ( 0 )
		)
		DirControl ( -1 0 1 1 )
		EmergencyStopToggle ( 0 1 0 )
		EmergencyStopResetToggle ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		Horn ( 0 1 0 )
		PantographToggle1 ( 0 1 0 )
		Sanding ( 0 1 0 )
		Vigilance ( 0 1 0 )
		Wipers ( 0 1 0 )
	)

	Name ( "BR 143-RB31 D-N (RA-BD)" )
	Sound ( "pt_143cab.sms" )

	Description (
		"Die BR 143 (ehemalige DR 243) ist eine elektrische Lokomotive, die nach der Wende von der DR übernommen wurde.\n\nThe BR 143 (former DR 143) is an electric locomotive, which was taken over by the DB from the DR.\n\nHersteller: LEW Hennigsdorf\n\nIndienststellung: 1984 \n\nStromquelle: Oberleitung 15kV/16,7Hz \n\nLeistung: 3720 Kilowatt\n\nHoechstgeschwindigkeit: 120 km/h\n\n" +
		"Max. Anfahrzugkraft: 240kN \n\n" +
		"Antriebsart: Kegelringfeder\n\n" +
		"Dienstmasse: 82,5t\n\n" +
		"Laenge ueber Puffer: 16.640mm \n\n" +
		"Radkonfiguration: Bo'Bo'\n\n" +
		"Typ: Electric Locomotive\n\n" +
		"Power source: cantenary wire, 15kV, 16 2/3 Hz\n\n" +
		"Power: 3.720 Kilowatt\n\n" +
		"Maximum Speed: 120 km/h (65 mph)\n\n" +
		"Weight: 82,8t\n\n" +
		"Max. temporary traction power: 240kN\n\n" +
		"Wheelset: Bo'Bo'"
	)
	EngineOperatingProcedures (
		"So setzen Sie den Zug in Bewegung\n1.	Drücken Sie die W-TASTE, um den Richtungshebel in die Position Vorwärts zu bringen.\n2.	Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n3.	Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n4.	Drücken Sie die D-TASTE, um den Regler von der Position Leerlauf in Kerbe 1 zu bewegen.\n5.	Erhöhen Sie die Leistung (D-TASTE) Kerbe für Kerbe, bis der Zug die gewünschte Geschwindigkeit erreicht hat.\n\nSo bremsen Sie den Zug ab\n1.	Drücken Sie die A-Taste, um den Regler in eine niedrigere Einstellung zu bewegen.\n" +
		"2.	Setzen Sie die Bremsen ein, wenn Sie noch weiter abbremsen möchten.\n\n" +
		"So bedienen Sie die Betriebsbremsen\n" +
		"1.	Drücken Sie die A-TASTE, um den Regler in die Position Leerlauf zu bewegen.\n" +
		"2.	Warten Sie zehn Sekunden, und drücken Sie dann die .-TASTE (Punkt), um den Hebel für die Betriebsbremse aus der Position Aus in die Position Leerlauf zu bewegen. Warten Sie einige Sekunden, bis der Bremskreislauf geschlossen ist, und drücken Sie die .-TASTE erneut, bis Sie die gewünschte Stufe für die Betriebsbremse (Stufen 1 bis 8) erreicht haben.\n\n" +
		"So lösen Sie die Betriebsbremsen\n" +
		"1. Drücken Sie die D-TASTE, um den Regler in Richtung Leerlauf zu bewegen.\n\n" +
		"So bedienen Sie die Zugbremsen\n" +
		"1.	Drücken Sie die Ä-TASTE, um die Zugbremse zu ziehen.\n\n" +
		"So lösen Sie die Zugbremsen auf der Lokomotive getrennt\n" +
		"1. Drücken Sie --TASTE (MINUS).\n\n" +
		"So lösen Sie die Zugbremsen\n" +
		"1. Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n\n" +
		"So betätigen Sie die Lokbremse\n" +
		"1.	Drücken Sie die +-TASTE (Pluszeichen), um die Lokbremse anzuziehen.\n\n" +
		"So lösen Sie die Lokbremse\n" +
		"1. Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n\n" +
		"So lösen Sie die Notbremse aus\n" +
		"1.	Drücken Sie die A-TASTE, um den Regler in die Position Leerlauf zu stellen.\n" +
		"2.	Drücken Sie die RÜCKTASTE, um die Notbremsung auszulösen.\n\n" +
		"So fahren Sie rückwärts\n" +
		"1.	Halten Sie den Zug vollständig an.\n" +
		"2.	Drücken Sie die S-TASTE, um den Richtungshebel in die Position Rückwärts zu stellen.\n" +
		"3.	Lösen Sie die Bremsen.\n" +
		"4.	Schieben Sie den Regler langsam nach vorne (D-TASTE).\n\n" +
		"So kuppeln Sie an einen Waggon oder eine Lokomotive an\n" +
		"1. Fahren Sie sehr langsam an die Einheit heran, mit etwa 2 km/h.\n" +
		"TIPP: Für die Kupplungsansicht drücken Sie die 6-Taste.\n" +
		"2. Drücken Sie F9, um das Zugbedienungsfenster zu öffnen.\n" +
		"3. Wenn das Symbol für die angekuppelte Einheit rot angezeigt wird, ist die Handbremse gezogen. Doppelklicken Sie auf den Waggon, um die Handbremse zu lösen.\n" +
		"4. Schließen Sie das Zugbedienungsfenster.\n\n" +
		"So kuppeln Sie von einem Waggon oder einer Lokomotive ab\n" +
		"1. Drücken Sie F9, um das Zugbedienungsfenster zu öffnen.\n" +
		"2. Doppelklicken Sie auf eine Einheit in dem Bereich des Zuges, den Sie von der Lokomotive abkuppeln möchten, um die Handbremse zu ziehen.\n" +
		"3. Doppelklicken Sie auf die Kupplung zwischen den Einheiten, die Sie vom Rest des Zuges abkuppeln möchten.\n" +
		"4. Schließen Sie das Fenster Zugbedienung."
	)
)
