SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RA-BD-DABuzf-D-N
	Type ( Engine )
	WagonShape ( "RA-BD-DABuzf-D.s" )
	Size ( 3.011m 4.507m 26.622m )
	Mass ( 44t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.011m 4.507m 26.622m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1E6N/m 5E6N/m )
			Damping ( 1E6N/m/s 1E6N/m/s )
			Break ( 6E7N 6E7N )
			r0 ( 15cm 1E9m )
		)
		CouplingHasRigidConnection (  )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1E6N/m 5E6N/m )
			Damping ( 1E6N/m/s 1E6N/m/s )
			r0 ( 0m 1E9m )
		)
		Centre ( 0.5m )
		Radius ( 1m )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.25 0.49 1.8 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 1290kN )
	DerailBufferForce ( 250kN )
	NumWheels ( 2 )
	Friction (
		50N/m/s	1	-1mph	0N/m/s	1
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)
	AntiSlip (  )
	BrakeEquipmentType ( "triple_valve,auxilary_reservoir,emergency_brake_reservoir" )
	BrakeSystemType ( Air_single_pipe )
	MaxBrakeForce ( 37.5kN )
	EmergencyBrakeResMaxPressure ( 145.038 )
	TripleValveRatio ( 2.5 )
	MaxReleaseRate ( 30 )
	MaxApplicationRate ( 25 )
	MaxAuxilaryChargingRate ( 20 )
	EmergencyResCapacity ( 10 )
	EmergencyResChargingRate ( 25 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 50.763 )
	FreightAnim ( "logo-STW-v.s" 1 1 )
	PassengerCapacity ( 122 )
	Lights ( 11
		Light (
			comment ( Lichtkegel #1 )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFB6926D )
					Position ( 0 1.5 20 )
					Angle ( 20 )
					Transition ( 0 )
					Radius ( 150 )
				)
			)
		)
		Light (
			comment ( Lichtkegel #2 )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFAD09F )
					Position ( 0 1.5 20 )
					Angle ( 25 )
					Transition ( 0 )
					Radius ( 200 )
				)
			)
		)
		Light (
			comment ( vorn mitte abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFADEBD )
					Position ( 0 2.218 12.9 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( vorn rechts abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFADEBD )
					Position ( -0.97 1.65 12.94 )
					Azimuth ( -9 -9 -9 )
					Elevation ( -11.5 -11.5 -11.5 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( vorn links abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFADEBD )
					Position ( 0.97 1.65 12.94 )
					Azimuth ( 9 9 9 )
					Elevation ( -11.5 -11.5 -11.5 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( vorn mitte aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( 0 2.218 12.9 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( vorn rechts aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( -0.97 1.65 12.94 )
					Azimuth ( -9 -9 -9 )
					Elevation ( -11.5 -11.5 -11.5 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( vorn links aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( 0.97 1.65 12.94 )
					Azimuth ( 9 9 9 )
					Elevation ( -11.5 -11.5 -11.5 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( AI vorn mitte  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( 0 2.218 12.9 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( AI vorn rechts  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				Weather ( 0 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( -0.97 1.65 12.94 )
					Azimuth ( -9 -9 -9 )
					Elevation ( -11.5 -11.5 -11.5 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( AI vorn links  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				Weather ( 0 )
			)
			FadeIn ( 0.2 )
			FadeOut ( 0.2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFD0 )
					Position ( 0.97 1.65 12.94 )
					Azimuth ( 9 9 9 )
					Elevation ( -11.5 -11.5 -11.5 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
	)
	Sound ( "StwOut.SMS" )
)

Engine ( RA-BD-DABuzf-D-N
	Wagon ( "RA-BD-DABuzf-D-N" )
	Type ( Electric )
	MaxPower ( 10kW )
	MaxForce ( 1kN )
	MaxContinuousForce ( 2kN )
	MaxVelocity ( 120km/h )
	MaxCurrent ( 1640A )
	WheelRadius ( 0.5m )
	Sanding ( 1E9mph )
	NumWheels ( 4 )

	HeadOut ( 1.85m 2.8m 11.5m )

	AirBrakesAirCompressorPowerRating ( 1.2 )
	AirBrakesAirCompressorWattage ( 10000 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.22 )
	AirBrakesCompressorRestartPressure ( 120 )
	AirBrakesIsCompressorElectricOrMechanical ( 1 )
	AirBrakesMainMaxAirPressure ( 145.038 )
	AirBrakesMainMinResAirPressure ( 0 )
	AirBrakesMainResVolume ( 8 )
	EngineBrakesControllerMinPressureReduction ( 6 )
	EngineBrakesControllerMaxApplicationRate ( 20 )
	EngineBrakesControllerMaxReleaseRate ( 15 )
	EngineBrakesControllerEmergencyApplicationRate ( 50 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 72.52 )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	EngineBrakesControllerFullServicePressureDrop ( 26 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	TrainBrakesControllerMinPressureReduction ( 6 )
	TrainBrakesControllerMaxApplicationRate ( 20 )
	TrainBrakesControllerMaxReleaseRate ( 4 )
	TrainBrakesControllerEmergencyApplicationRate ( 50 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 72.52 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerFullServicePressureDrop ( 26 )
	EngineBrakesProportionalBrakeLag ( 0.9 )

	DynamicBrakesMinUsableSpeed ( 2 )
	DynamicBrakesMaximumEffectiveSpeed ( 31 )
	DynamicBrakesMaximumForce ( 200kN )
	DynamicBrakesResistorCurrentLimit ( 5000 )
	DynamicBrakesCutInSpeed ( 1 )
	DynamicBrakesMaxAirBrakePressure ( 15 )
	DynamicBrakesFadingSpeed ( 5 )
	DynamicBrakesDelayTimeBeforeEngaging ( 3 )
	DynamicBrakesMaximumSpeedForFadeOut ( 100 )
	DynamicBrakesEffectAtMaximumFadeOut ( 1 )
	DynamicBrakesHigherSpeedCurveExponent ( 1 )
	DynamicBrakesLowerSpeedCurveExponent ( 1 )
	DynamicBrakesNumberOfControllerNotches ( 10 )
	BrakesEngineBrakeType ( Air_single_pipe )
	BrakesTrainBrakeType ( Air_single_pipe )
	BrakesEngineControllers ( "Train,Independent,Dynamic" )
	DoesBrakeCutPower ( 1 )

	CabView ( "Nacht\\pt_dbmq-n.cvf" )

	DoesHornTriggerBell ( 0 )

	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 45 )
		MonitoringDeviceAlarmTimeLimit ( 30 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
	)
	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnResetButton ( 1 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 300 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
		MonitoringDeviceResetOnResetButton ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
	)

	EngineControllers (
		BailOffButton ( 0 1 0 )
		BellToggle ( 0 1 0 )
		Brake_Dynamic ( 0 1 0.11 0
			NumNotches ( 10
				Notch ( 0 0 Dummy )
				Notch ( 0.11 0 Dummy )
				Notch ( 0.22 0 Dummy )
				Notch ( 0.33 0 Dummy )
				Notch ( 0.44 0 Dummy )
				Notch ( 0.55 0 Dummy )
				Notch ( 0.66 0 Dummy )
				Notch ( 0.77 0 Dummy )
				Notch ( 0.88 0 Dummy )
				Notch ( 1 0 Dummy )
			)
		)
		Brake_Engine ( 0 1 0.025 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Train ( 0 1 0.0125 0.28
			NumNotches ( 6
				Notch ( 0 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.2 0 TrainBrakesControllerHoldLappedStart )
				Notch ( 0.25 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.85 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.9 0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
			)
		)
		Throttle ( 0 1 0.025 0
			NumNotches ( 0 )
		)
		DirControl ( -1 0 1 1 )
		EmergencyStopToggle ( 0 1 0 )
		EmergencyStopResetToggle ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		Horn ( 0 1 0 )
		PantographToggle1 ( 0 1 0 )
		Sanding ( 0 1 0 )
		Vigilance ( 0 1 0 )
		Wipers ( 0 1 0 )
	)

	Name ( "DABuzf-F-RB31 D-N (RA-BD)" )
	Sound ( "StwIn.SMS" )

	Description (
		"Da auch nach der Beschaffung der DBmqz 773 bis 1991 immer noch ein Mangel \nan Steuerwagen herrschte,entschloß sich die DR 1992/93 eine weitere Serie \nDoppelstock-Steuerwagen in Dienst zu stellen. Allerdings unterschieden sich \ndie Wagen in der Kopfform deutlich von ihren Vorgängers.Auch wurden der seitliche \nDachbereich erweitert und im Oberstock gekrümmte Scheiben eingebaut \nInsgesammt lieferte die Waggonbau Görlitz 100 Fahrzeuge dieses Typs.\n1998 waren sie u.a in Leipzig,Rostock,Dresden,Magdeburg,Berlin und \n" +
		"Stuttgart beheimatet\n\n" +
		"Länge : 26.8 m \n" +
		"Dienstmasse :  48.000 kg\n" +
		"Höchstgeschwindigkeit: 140 km/h"
	)
	EngineOperatingProcedures (
		"So setzen Sie den Zug in Bewegung\n1.	Drücken Sie die W-TASTE, um den Richtungshebel in die Position Vorwärts zu bringen.\n2.	Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n3.	Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n4.	Drücken Sie die D-TASTE, um den Regler von der Position Leerlauf in Kerbe 1 zu bewegen.\n5.	Erhöhen Sie die Leistung (D-TASTE) Kerbe für Kerbe, bis der Zug die gewünschte Geschwindigkeit erreicht hat.\n\nSo bremsen Sie den Zug ab\n" +
		"1.	Drücken Sie die A-Taste, um den Regler in eine niedrigere Einstellung zu bewegen.\n" +
		"2.	Setzen Sie die Bremsen ein, wenn Sie noch weiter abbremsen möchten.\n\n" +
		"So bedienen Sie die Betriebsbremsen\n" +
		"1.	Drücken Sie die A-TASTE, um den Regler in die Position Leerlauf zu bewegen.\n" +
		"2.	Warten Sie zehn Sekunden, und drücken Sie dann die .-TASTE (Punkt), um den Hebel für die Betriebsbremse aus der Position Aus in die Position Leerlauf zu bewegen. Warten Sie einige Sekunden, bis der Bremskreislauf geschlossen ist, und drücken Sie die .-TASTE erneut, bis Sie die gewünschte Stufe für die Betriebsbremse (Stufen 1 bis 8) erreicht haben.\n\n" +
		"So lösen Sie die Betriebsbremsen\n" +
		"1. Drücken Sie die D-TASTE, um den Regler in Richtung Leerlauf zu bewegen.\n\n" +
		"So bedienen Sie die Zugbremsen\n" +
		"1.	Drücken Sie die Ä-TASTE, um die Zugbremse zu ziehen.\n\n" +
		"So lösen Sie die Zugbremsen auf der Lokomotive getrennt\n" +
		"1. Drücken Sie --TASTE (MINUS).\n\n" +
		"So lösen Sie die Zugbremsen\n" +
		"1. Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n\n" +
		"So betätigen Sie die Lokbremse\n" +
		"1.	Drücken Sie die +-TASTE (Pluszeichen), um die Lokbremse anzuziehen.\n\n" +
		"So lösen Sie die Lokbremse\n" +
		"1. Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n\n" +
		"So lösen Sie die Notbremse aus\n" +
		"1.	Drücken Sie die A-TASTE, um den Regler in die Position Leerlauf zu stellen.\n" +
		"2.	Drücken Sie die RÜCKTASTE, um die Notbremsung auszulösen.\n\n" +
		"So fahren Sie rückwärts\n" +
		"1.	Halten Sie den Zug vollständig an.\n" +
		"2.	Drücken Sie die S-TASTE, um den Richtungshebel in die Position Rückwärts zu stellen.\n" +
		"3.	Lösen Sie die Bremsen.\n" +
		"4.	Schieben Sie den Regler langsam nach vorne (D-TASTE).\n\n" +
		"So kuppeln Sie an einen Waggon oder eine Lokomotive an\n" +
		"1. Fahren Sie sehr langsam an die Einheit heran, mit etwa 2 km/h.\n" +
		"TIPP: Für die Kupplungsansicht drücken Sie die 6-Taste.\n" +
		"2. Drücken Sie F9, um das Zugbedienungsfenster zu öffnen.\n" +
		"3. Wenn das Symbol für die angekuppelte Einheit rot angezeigt wird, ist die Handbremse gezogen. Doppelklicken Sie auf den Waggon, um die Handbremse zu lösen.\n" +
		"4. Schließen Sie das Zugbedienungsfenster.\n\n" +
		"So kuppeln Sie von einem Waggon oder einer Lokomotive ab\n" +
		"1. Drücken Sie F9, um das Zugbedienungsfenster zu öffnen.\n" +
		"2. Doppelklicken Sie auf eine Einheit in dem Bereich des Zuges, den Sie von der Lokomotive abkuppeln möchten, um die Handbremse zu ziehen.\n" +
		"3. Doppelklicken Sie auf die Kupplung zwischen den Einheiten, die Sie vom Rest des Zuges abkuppeln möchten.\n" +
		"4. Schließen Sie das Fenster Zugbedienung."
	)
)
