SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 371001
	Type ( Engine )
	WagonShape ( 371001.s )

	Comment ( Eng created by ZSR - http://csd.webzdarma.cz )
	Comment ( Datum: 3/3/2009 )
	Comment ( Version: 1.07 )
	Comment ( Brzdic provizorne nastaven na BSE vzhledem k neexistenci kabiny s BS2 )
	Comment ( Mez adheze: 187kN = 980A  )
	Comment ( Mez adheze piskovan: 225kN )
	Comment ( Nadproudovy ochrana = 850A ) 
	
comment	( Overall physics )

	Size ( 3.00m 4.69m 16.542m )
	CentreOfGravity ( 0m 2.25m 0m )
	Mass ( 84t )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box (3.00m 4.69m 16.542m) )

comment	( Coupling )

comment ( Rear Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 30cm 60cm )
		)
	CouplingHasRigidConnection ( 0 )
	Velocity ( 0.01m/s )
	)
	

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	
comment	( Adhesion and Friction )

	Adheasion ( 0.114 0.79 1.15 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*84t )
	DerailBufferForce ( 800kN )
	NumWheels (	4 )
	Friction (
		2500N/m/s		0		10mph		15N/m/s		2.14
		5.1N/rad/s		1		-1rad/s		0		1
	)

comment	( Wagon Brakes )

 	Comment ( P=44kN, G=24kN )
 	
	MaxBrakeForce( 44kN )
	MaxHandbrakeForce( 30kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.3 )
	MaxApplicationRate( 4 )
	MaxAuxilaryChargingRate( 3 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 11 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 )
	
comment	( EngSound, Freight, Inside, IntakePoint )

	Sound ( "../../common.snd/sndelok/372eng.sms" )
	Comment ( "../../Zvuky/loko_elektr/371eng.sms" )
	
   	
	Inside (
		PassengerCabinFile ( 371001.s )
		PassengerCabinHeadPos ( -1.7 3.1 5.9 )
		RotationLimit ( 0 190 0 )
		StartDirection ( 0 180 0 )
	)

comment	( Lights )
	Lights ( 19
	Light (
	comment ( Lichtschein )
	Type ( 1 )
	Conditions (
        	Headlight ( 4 )
		Unit ( 2 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( 0 1 8 )
		Angle ( 15 )
		Radius ( 100 )
		)
	)
)
        Light (
	comment ( Mitte li )
	Type ( 0 )
       	Conditions (
		Headlight ( 3 )
		Unit ( 2 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( -0.1 2.54 7.95 )
		Azimuth ( 0 0 0 )
		Radius ( 0.4 )
		Elevation ( -3 -3 -3 )
		)
	)
)
	Light (
	comment ( Mitte re )
	Type ( 0 )
	Conditions (
		Headlight ( 3 )
		Unit ( 2 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( 0.1 2.54 7.95 )
		Azimuth ( 0 0 0 )
		Radius ( 0.4 )
		Elevation ( -3 -3 -3 )
		)
	)
)
        Light (
	comment ( links )
	Type ( 0 )
	Conditions (
                Headlight ( 4 )
        	Unit ( 2 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( -0.75 1.67 7.84 )
		Azimuth ( 0.0 0.0 0.0 )
		Radius ( 0.5 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light (
	comment ( rechts )
	Type ( 0 )
	Conditions (
		Headlight ( 4 )
		Unit ( 2 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( 0.75 1.67 7.84 )
		Azimuth ( 0 0 0 )
		Radius ( 0.5 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light (
	comment ( links rot )
	Type ( 0 )
	Conditions (
		Unit ( 3 )
		Service ( 2 )
		)
	States ( 1
		State (
		LightColour ( FFFF0000 )
		Position ( -1.00 1.67 -7.84 )
		Azimuth ( 180 180 180 )
		Radius ( 0.4 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light (
	comment ( rechts rot )
	Type ( 0 )
	Conditions (
		Unit ( 3 )
		Service ( 2 )
		)
	States ( 1
		State (
		LightColour ( FFFF0000 )
		Position ( 1.00 1.67 -7.84 )
		Azimuth ( 180 180 180 )
		Radius ( 0.4 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light (
	comment ( Mitte re rev )
	Type ( 0 )
	Conditions (
		Headlight ( 3 )
		Unit ( 5 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( 0.1 2.54 -7.95 )
		Azimuth ( 180 180 180 )
		Radius ( 0.4 )
		Elevation ( -3 -3 -3 )
		)
	)
)
	Light (
	comment ( Mitte li rev )
	Type ( 0 )
	Conditions (
		Headlight ( 3 )
		Unit ( 5 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( -0.1 2.54 -7.95 )
		Azimuth ( 180 180 180 )
		Radius ( 0.4 )
                Elevation ( -3 -3 -3 )
		)
	)
)
        Light (
	comment ( rechts rev )
	Type ( 0 )
	Conditions (
		Headlight ( 4 )
		Unit ( 5 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( 0.75 1.67 -7.84 )
		Azimuth ( 180 180 180 )
		Radius ( 0.5 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light (
	comment ( links rev )
	Type ( 0 )
	Conditions (
		Headlight ( 4 )
		Unit ( 5 )
		)
		FadeIn ( 1.5 )
		FadeOut ( 1.5 )
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( -0.75 1.67 -7.84 )
		Azimuth ( 180 180 180 )
		Radius ( 0.5 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light (
	comment ( rechts rot rev )
	Type ( 0 )
	Conditions (
		Unit ( 4 )
		Service ( 2 )
		)
	States ( 1
		State (
		LightColour ( FFFF0000 )
		Position ( 1.00 1.67 7.84 )
		Azimuth ( 0 0 0 )
		Radius ( 0.4 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light (
	comment ( links rot rev )
	Type ( 0 )
	Conditions (
		Unit ( 4 )
		Service ( 2 )
		)
	States ( 1
		State (
		LightColour ( FFFF0000 )
		Position ( -1.00 1.67 7.84 )
		Azimuth ( 0 0 0 )
		Radius ( 0.4 )
		Elevation ( 8 8 8 )
		)
	)
)
        Light (
	comment ( KI Mitte li )
	Type ( 0 )
       	Conditions (
		Service ( 2 )
		Unit ( 2 )
		Control ( 1 )
		TimeOfDay ( 2 )
		)
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( -0.1 2.54 7.95 )
		Azimuth ( 0 0 0 )
		Radius ( 0.4 )
		Elevation ( -3 -3 -3 )
		)
	)
)
	Light (
	comment ( KI Mitte re )
	Type ( 0 )
	Conditions (
		Service ( 2 )
		Unit ( 2 )
		Control ( 1 )
		TimeOfDay ( 2 )
		)
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( 0.1 2.54 7.95 )
		Azimuth ( 0 0 0 )
		Radius ( 0.4 )
		Elevation ( -3 -3 -3 )
		)
	)
)
        Light (
	comment ( KI links )
	Type ( 0 )
	Conditions (
		Service ( 2 )
		Unit ( 2 )
		Control ( 1 )
		TimeOfDay ( 2 )
		)
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( -0.75 1.67 7.84 )
		Azimuth ( 0.0 0.0 0.0 )
		Radius ( 0.5 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light (
	comment ( KI rechts )
	Type ( 0 )
	Conditions (
		Service ( 2 )
		Unit ( 2 )
		Control ( 1 )
		TimeOfDay ( 2 )
		)
	States ( 1
		State (
		LightColour ( fffaf8aa )
		Position ( 0.75 1.67 7.84 )
		Azimuth ( 0 0 0 )
		Radius ( 0.5 )
		Elevation ( 8 8 8 )
		)
	)
)
	Light	(
	comment  ( Bügelfeuer Schnee )
	Type ( 0 )
	Conditions (
		Service ( 2 )
		Weather ( 3 )
		)
		Cycle	( 0 )
	States	( 8
		State	(
		Duration ( 5.0 )
		LightColour ( 00000000 )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.6 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 0.2 )
		LightColour ( ff00ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.2 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 0.1 )
		LightColour ( 8000ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.4 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 4.0 )
		LightColour ( 00000000 )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.6 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 0.2 )
		LightColour ( 8000ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.8 )
		Elevation ( 0.0 0.0 0.0 )
		)
        	State	(
		Duration ( 0.3 )
		LightColour ( ff00ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 3.0 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 3.0 )
		LightColour ( 00000000 )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.6 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 0.2 )
		LightColour ( ff00ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.8 )
		Elevation ( 0.0 0.0 0.0 )
		)
	)
)
	Light	(
	comment  ( Bügelfeuer )
	Type ( 0 )
	Conditions (
		Service ( 2 )
		)
		Cycle	( 0 )
	States	( 8
		State	(
		Duration ( 90.0 )
		LightColour ( 00000000 )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.6 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 0.2 )
		LightColour ( ff00ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.8 )
		Elevation ( 0.0 0.0 0.0 )
		)
        	State	(
		Duration ( 0.1 )
		LightColour ( 8000ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.6 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 55.0 )
		LightColour ( 00000000 )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.6 )
        	Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 0.2 )
		LightColour ( 8000ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.7 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 0.1 )
		LightColour ( ff00ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 3.0 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 75.0 )
		LightColour ( 00000000 )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.5 )
		Elevation ( 0.0 0.0 0.0 )
		)
		State	(
		Duration ( 0.1 )
		LightColour ( ff00ccff )
		Position ( 0.0 6.0 -3.95 )
		Azimuth ( 0.0 -180.0 180.0 )
		Transition ( 0 )
		Radius ( 0.4 )
		Elevation ( 0.0 0.0 0.0 )
		)
	)
)
)
)

Engine ( 371001

comment	( Description )

	Wagon ( 371001 )

	
comment	( Basic physical engine data )

	Type ( Electric )
	MaxPower ( 4466kW )
	MaxForce ( 1638kN )	
	MaxContinuousForce ( 1638kN )
	MaxCurrent ( 8583A ) 
	MaxVelocity ( 99.4mph )
	DieselEngineSpeedOfMaxTractiveEffort( 0mph )  
	WheelRadius ( 0.625m )
	comment( sanding system is switched off when faster than given velocity )
	Sanding ( 1e9mph )
	NumWheels ( 4 )

	
comment	( CabSound and Views )

	Sound ( "../../common.snd/sndelok/372cab.sms" )
	Comment ( "../../Zvuky/loko_elektr/371cab.sms" )

	CabView ( "../../common.cab/cab362/362.cvf" )
	HeadOut (1.7 3.1 5.9 )
	


comment	( Brakes )


	AirBrakesAirCompressorPowerRating ( 1.18 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 145 )	
	AirBrakesMainResVolume ( 31.783 )
	AirBrakesAirCompressorWattage ( 15000 )
	AirBrakesCompressorRestartPressure ( 102 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1 )
	TrainBrakesControllerMaxReleaseRate ( 0.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 1.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 3 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 )
	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )

	 
	 DynamicBrakesResistorCurrentLimit    ( 480 )
	 DynamicBrakesDelayTimeBeforeEngaging   ( 4 )
	 DynamicBrakesNumberOfControllerNotches   ( 20 )
	 DynamicBrakesMaxAirBrakePressure    ( 20 )
	 DynamicBrakeHasAutoBailOff      ( 0 )
	 DynamicBrakesMaximumForce      ( 99kN )
	 DynamicBrakesLowerSpeedCurveExponent   ( 1.7 )
	 DynamicBrakesMinUsableSpeed      ( 12.43 )
	 DynamicBrakesFadingSpeed      ( 43.5 )
	 DynamicBrakesMaximumEffectiveSpeed    ( 43.5 )
	 DynamicBrakesMaximumSpeedForFadeOut    ( 472.4 )
	 DynamicBrakesEffectAtMaximumFadeOut    ( 0 )
	 DynamicBrakesCutInSpeed       ( 12.43 )
	 DynamicBrakesCutOutSpeed       ( 12.43 )
	 DynamicBrakesHigherSpeedCurveExponent   ( 6 )

	 BrakesEngineBrakeType( "Air_single_pipe"  )
	 BrakesTrainBrakeType( "Air_single_pipe" )
	 BrakesEngineControllers( "Independent, Train, Dynamic" )

	 DoesBrakeCutPower ( 1 )

comment ( Monitors )


EmergencyStopMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 0 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  
 )
 VigilanceMonitor (
  MonitoringDeviceMonitorTimeLimit ( 27 )
  MonitoringDeviceAlarmTimeLimit ( 17 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 )
  MonitoringDeviceResetOnResetButton ( 1 )
  MonitoringDeviceResetOnDirectionNeutral ( 1 )
 )
 OverspeedMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 5 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 99.5 )
  MonitoringDeviceResetLevel ( 0 )
  Comment ( MonitoringDeviceTriggerOnHighCurrent ( 850 ) )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 0 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
  MonitoringDeviceDoesSuppressionReset ( 0 )
  MonitoringDeviceTriggerOnOverspeed ( 99.6 )
  MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 0 )
 )
		
	 
Comment	( Controllers )

        EngineControllers (
		Throttle ( 0 1 0.005 0
			NumNotches ( 12
			Notch ( 0.0   0 Dummy )
			Notch ( 0.05  0 Dummy )
			Notch ( 0.10  0 Dummy )
			Notch ( 0.20  0 Dummy )
			Notch ( 0.30  0 Dummy )
			Notch ( 0.40  0 Dummy )
			Notch ( 0.50  0 Dummy )
			Notch ( 0.60  0 Dummy )
			Notch ( 0.70  0 Dummy )
			Notch ( 0.80  0 Dummy )			
			Notch ( 0.90  0 Dummy )
			Notch ( 1     0 Dummy )
	) 
	)
		comment (***Primocinna brzda typ DAKO-BP***)
		Brake_Engine ( 0 1 0.05 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )                   
                )
            )
            comment (***Prubezna brzda typ DAKO-BSE***)
		Brake_Train 	( 0 1 0.05 0.8
			NumNotches ( 5
				Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.4 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.6 0 TrainBrakesControllerApplyStart )
				Notch ( 0.8 0 TrainBrakesControllerContinuousServiceStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)

            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            Brake_Dynamic  ( 0 1 0.1 0
	       NumNotches ( 1
	        Notch ( 0 1 Dummy )
	       		)
  		)
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            PantographToggle2  ( 0 1 0 )
            PantographsToggle_4  ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
	
Comment	( Operations )

	 Name ( " CD 371 001-6 Lucka" )
	 Description (
	 "Ovladani\n\n"+ 
	 "Lokomotiva ma oba sberace ovladatelne pomoci 4-polohoveho prepinace s koncovou polohou, ovlada se standardne klavesou P\n\n"+ 
	 "Vykon 39% odpovida hospodarnemu seriovemu stupni\n\n"+ 
	 "Vykon 79% odpovida hospodarnemu serioparalelnimu stupni\n\n"+
	 "Po kazdem hospodarne stupni nasleduji 5 stupnu shuntovacich a pak se kontroler vraci zpet postupne na hospodarny stupen\n\n"+
	"Pretizeni:\n"+
	"Proud trvaly : 548A\n\n"+
    	"Proud 60min: 611A\n\n"+
      "Nadproudova ochrana: 850A\n\n"+
	"Brzdic prubezne vlakove brzdy DAKO BS2\n\n"+
	"Brzdic lokomotivni brzdy DAKO-BP\n\n"+
	"Rada 371 CD je univerzalni elektricka skrinova lokomotiva, pouzivana v nakladni i osobni doprave.\n"+
	"Typ Bo'-Bo', napeti 3kV ss, 15kV 16 2/3Hz.\n\n"+
	"Delka pres narazniky: 16,8 m\n\n"+
	"Prumer hnacich kol: 1250 mm\n\n"+
	"Hmotnost ve sluzbe: 84 t\n\n"+
	"Trvaly vykon trakcnich motoru: 3080 kW ss/3060 kW st\n\n"+
	"Max. rychlost 160 km/h\n\n"
    	)

   	EngineOperatingProcedures (
		"Stupne kontroleru:\n"+
		"1.-27.	( 0 - 37%) Rozjezdove stupne seriove\n"+
		"28.	(39%)      Hospodarny seriovy stupen (odporniky vyrazeny)\n"+
		"I.-V.	(40 - 47%) Shuntovaci rozjedove stupne, vsechny motory v serii\n"+
		"B.     (40%)	   Prechodovy stupen S - SP\n"+
		"29.-46.(41 - 78%) Odporove serio-paralelni stupne (vzdy dva motory v serii)\n"+		
		"47.	(79%)      Hospodarny serio-paralelni stupen (odporniky vyrazeny)\n"+
		"I.-V.	(84 - 100%)Shuntovaci stupne pro paralelni zapojeni motoru\n\n"		
	)
)