SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( TM_120_367
	Type ( Engine )
	WagonShape ( TM_120_367.s )
	Size ( 2.95m 4.493m 17.72m)
	Mass ( 116.5t )
	WheelRadius ( 0.525m )
	InertiaTensor ( Box ( 3.0m 4.71m 17.55m )
 	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1E7N/m 1E7N/m )
			Damping ( 1E6N/m 1E6N/m )
			R0 ( 0cm 10cm )
			Break ( 5.2E7N 5.2E7N )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 5E6N/m 5E6N/m )
			Damping ( 1E6N/m/s 1E6N/m/s )
			R0 ( 0cm 10cm )
		)
		Centre ( 0.5m )
		Radius ( 1m )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.3 0.5 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 288KN )
	DerailBufferForce ( 1000kN )
	NumWheels ( 0 )
	Friction (
		1516N/m/s	0	1mph              12.93N/m/s     1.8
		0N/rad/s	1	-1rad/s		0	        1
                )
	AntiSlip ()
	
	BrakeEquipmentType( "graduated_release_triple_valve , Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 118kN )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 40 )
	MaxApplicationRate( 30 )
	MaxAuxilaryChargingRate( 116 )
	EmergencyResCapacity( 25 )
	EmergencyResChargingRate( 25 )
	EmergencyBrakeResMaxPressure( 70 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

	IntakePoint ( 1.06m 1.0m FuelDiesel )
	Sound ( "PT9-DR-120-185eng.sms" )
	Lights ( 14
		Light (
			comment ( Sphere of light)
			Type ( 1)
			Conditions (
				Headlight ( 3)
				Unit ( 2)
			)
			Cycle ( 0)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( 40ffffbb)
					Position ( 0.0 3.5 18)
					Transition ( 0)
					Radius ( 200.0)
					Angle ( 10.0)
				)
			)
		)
		Light (
			comment ( Head light left dim)
			Type ( 0)
			Conditions (
				Headlight ( 2)
				Unit ( 2)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( 80ffffbb)
					Position ( 1.07 1.56 8.15)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 0.75)
					Elevation ( 0.0 0.0 0.0)
				)
			)
		)
		Light (
			comment ( Head light right dim)
			Type ( 0)
			Conditions (
				Headlight ( 2)
				Unit ( 2)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( 80ffffbb)
					Position ( -1.07 1.56 8.15)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 0.75)
					Elevation ( 0.0 0.0 0.0)
				)
			)
		)
		Light (
			comment ( Head Light Top Dim)
			Type ( 0)
			Conditions (
				Headlight ( 2)
				Unit ( 2)
			)
			Cycle ( 0)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( 80ffffbb)
					Position ( 0.0 4.17 8.1)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 1.0)
				)
			)
		)
		Light (
			comment ( Head Light Top Bright)
			Type ( 0)
			Conditions (
				Headlight ( 3)
				Unit ( 2)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( ffffffff)
					Position ( 0.0 4.17 8.1)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 1.0)
				)
			)
		)
		Light (
			comment ( Head light left Bright)
			Type ( 0)
			Conditions (
				Headlight ( 3)
				Unit ( 2)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( ffffffbb)
					Position ( 1.07 1.56 8.15)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 0.75)
					Elevation ( 0.0 0.0 0.0)
				)
			)
		)
		Light (
			comment ( Head light right Bright)
			Type ( 0)
			Conditions (
				Headlight ( 3)
				Unit ( 2)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( ffffffbb)
					Position ( -1.07 1.56 8.15)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 0.75)
					Elevation ( 0.0 0.0 0.0)
				)
			)
		)
		Light (
			comment ( Rear Head light left Red)
			Type ( 0)
			Conditions (
				Headlight ( 3)
				Unit ( 3)
				Coupling ( 2)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( 90ff0000)
					Position ( 1.3 1.56 -8.12)
					Azimuth ( -180 -180 -180)
					Transition ( 0)
					Radius ( 0.75)
					Elevation ( 0.0 0.0 0.0)
				)
			)
		)
		Light (
			comment ( Rear Head light right Red)
			Type ( 0)
			Conditions (
				Headlight ( 3)
				Unit ( 3)
				Coupling ( 2)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( 90ff0000)
					Position ( -1.3 1.56 -8.12)
					Azimuth ( -180 -180 -180)
					Transition ( 0)
					Radius ( 0.75)
					Elevation ( 0.0 0.0 0.0)
				)
			)
		)
		Light (
			comment ( AI)
			comment ( Head Light Top Bright)
			Type ( 0)
			Conditions (
				Headlight ( 3)
				Unit ( 2)
				Control ( 1)
				Service ( 2)
				TimeOfDay ( 0)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( ffffffff)
					Position ( 0.0 4.17 8.1)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 1.0)
				)
			)
		)
		Light (
			comment ( Head light left Bright)
			Type ( 0)
			Conditions (
				Headlight ( 3)
				Unit ( 2)
				Control ( 1)
				Service ( 2)
				TimeOfDay ( 0)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( ffffffbb)
					Position ( 1.07 1.56 8.15)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 0.75)
					Elevation ( 0.0 0.0 0.0)
				)
			)
		)
		Light (
			comment ( Head light right Bright)
			Type ( 0)
			Conditions (
				Headlight ( 3)
				Unit ( 2)
				Control ( 1)
				Service ( 2)
				TimeOfDay ( 0)
			)
			FadeIn ( 0.5)
			FadeOut ( 0.5)
			Cycle ( 0)
			States ( 1
				State (
					Duration ( 0.0)
					LightColour ( ffffffbb)
					Position ( -1.07 1.56 8.15)
					Azimuth ( 0.0 0.0 0.0)
					Transition ( 0)
					Radius ( 0.75)
					Elevation ( 0.0 0.0 0.0)
				)
			)
		)
	)
)
Engine ( TM_120_367
	
	Effects
		(
		DieselSpecialEffects
			(
				comment
				(
					the format of these little blocks is as follow:

					offset.x offset.y offset.z
					normal.x normal.y normal.z
					width in metres

					defining the offset from the shape pivot point
					where steam / smoke should appear, the direction
					it should go and the width of the nozzle
				)

				Exhaust1
				(
					0.2 4.61 -1.55
					0 0.9 0
					0.1
				)
                        Exhaust2
				(
					-0.2 4.61 -1.55
					0 1 0
					0.1
				)
			)
        	)
      Wagon ( TM_120_367 )
	Type ( Diesel )
	MaxPower ( 1672kW )
	MaxForce ( 420kN )
	MaxContinuousForce ( 360kN )
	MaxVelocity ( 100kmh )
	MaxCurrent ( 3570A )
	WheelRadius ( 0.525m )
	Vigilance ( 1 )
	Sanding ( 1e9mph )
	NumWheels ( 6 )
	MaxTemperature ( 90 )
	MaxOilPressure ( 90 )

	CabView ( PT_V200_DR.cvf )
	HeadOut ( 1.72 3.56 6.80 )
	
	AirBrakesAirCompressorPowerRating ( 300 )
	AirBrakesAirCompressorWattage ( 30000 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.1 )
	AirBrakesCompressorRestartPressure ( 135 )
	AirBrakesIsCompressorElectricOrMechanical ( 1 )
	AirBrakesMainMaxAirPressure ( 140 )
	AirBrakesMainMinResAirPressure ( 0 )
	AirBrakesMainResVolume ( 30 )

	EngineBrakesControllerMinPressureReduction ( 7 )
	EngineBrakesControllerMaxApplicationRate ( 40 )
	EngineBrakesControllerMaxReleaseRate ( 50 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 110 )
      EngineBrakesControllerEmergencyApplicationRate ( 50 )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	EngineBrakesControllerFullServicePressureDrop ( 50 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerDirectControlExponent ( 1 )
      EngineBrakesProportionalBrakeLag( 0.1 )
               
	TrainBrakesControllerMinPressureReduction ( 6 )
	TrainBrakesControllerMaxApplicationRate ( 40 )
	TrainBrakesControllerMaxReleaseRate ( 50 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 110 )
	TrainBrakesControllerMaxQuickReleaseRate ( 80 )
      TrainBrakesControllerEmergencyApplicationRate ( 50 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerFullServicePressureDrop ( 50 )
	
    DynamicBrakesMinUsableSpeed( 3 )
    DynamicBrakesMaximumEffectiveSpeed( 3 )
    DynamicBrakesMaximumForce( 177KN )
    DynamicBrakesResistorCurrentLimit ( 5000 )
    DynamicBrakesCutInSpeed( 3 )
    DynamicBrakesMaxAirBrakePressure ( 50 )
    DynamicBrakesFadingSpeed( 70 )
    DynamicBrakesDelayTimeBeforeEngaging ( 0 )
    DynamicBrakesMaximumSpeedForFadeOut ( 70 )
    DynamicBrakesEffectAtMaximumFadeOut( 0 )
    DynamicBrakesHigherSpeedCurveExponent( 1 )
    DynamicBrakesLowerSpeedCurveExponent( 1 )
    DynamicBrakesNumberOfControllerNotches( 0 )

    BrakesEngineBrakeType ( Air_single_pipe )
    BrakesTrainBrakeType ( Air_single_pipe )
    BrakesEngineControllers( "Independent, Train, Dynamic" )

	MaxDieselLevel ( 3900l )
	DieselUsedPerHourAtMaxPower ( 180l )
	DieselUsedPerHourAtIdle ( 18l )

	DieselSmokeEffectInitialMagnitude( 0.5 )
	DieselSmokeEffectMaxMagnitude( 9 )
	DieselSmokeEffectInitialSmokeRate( 0.5 )
	DieselSmokeEffectMaxSmokeRate( 10 )

	DieselEngineIdleRPM ( 400 )
	DieselEngineMaxRPM ( 750 )
	DieselEngineSpeedOfMaxTractiveEffort ( 20kmh )
	DieselEngineMaxRPMChangeRate ( 95 )
	
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 60 )
		MonitoringDeviceAlarmTimeLimit ( 40 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 100 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
	)
	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 100 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
	)
	EngineControllers (
		Throttle ( 0 1 0.1 0
		NumNotches ( 12
			Notch ( 0.00   0 Dummy )
			Notch ( 0.05   0 Dummy )
			Notch ( 0.10   0 Dummy )
			Notch ( 0.20   0 Dummy )
			Notch ( 0.30   0 Dummy )
			Notch ( 0.40   0 Dummy )
			Notch ( 0.50   0 Dummy )
			Notch ( 0.60   0 Dummy )
			Notch ( 0.70   0 Dummy )
			Notch ( 0.80   0 Dummy )
			Notch ( 0.90   0 Dummy )
			Notch ( 1.00   0 Dummy )
			)
		)
	Brake_Engine ( 0 1 0.03 0
		NumNotches ( 1
			Notch ( 0 1 Dummy )
			)
		)
	Brake_Train ( 0 1 0.025 0.35
		NumNotches ( 5
		Notch ( 0      0 TrainBrakesControllerReleaseStart )
		Notch ( 0.3   1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
		Notch ( 0.85 0 TrainBrakesControllerSuppressionStart )
		Notch ( 0.9   0 TrainBrakesControllerContinuousServiceStart )
		Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
		)
	)
            Brake_Dynamic ( 0 1 0.04 0 
              	NumNotches ( 0
                  	)
            )
	DirControl ( -1 0 1 1 )
	BellToggle ( 0 1 0 )
	Sanding ( 0 1 0 )
	Horn ( 0 1 0 )
	Wipers ( 0 1 0 )
	EmergencyStopToggle ( 0 1 0 )
	Vigilance ( 0 1 0 )
	Headlights ( 0 0.25 1 0 )
	)
	EngineVariables ( 3900 )
	Sound ( "PT9-DR-120-185cab.sms" )
	Name ( "TM_BR 120 367-7 BW Dresden" )
	Description ( 
	"Technische Daten BR 120 ´Taigatrommel´: \n\n"+
	"Lokomotivtyp: Dieselelektrische Gueterzuglokomotive \n\n"+
	"Hersteller: Diesellokomotivfabrik ´Oktoberrevolution´ Woroschilowgrad (UdSSR) \n\n"+
	"Baujahre: 1966 bis 1975 \n\n"+
	"Exemplare: 378 fuer die Deutsche Reichsbahn \n\n"+	
	"Motortyp: 12 Zylinder 2-Takt V-Motor 14D40\n\n"+
	"Leistung: 1470 kW/ 2000 PS \n\n"+
	"Achsanordnung: Co'Co' \n\n"+ 
	"Hoechstgeschwindigkeit: 100 km/h \n\n"+
	"Gewicht: 115,1 t \n\n"+
	"Anfahrzugkraft: 320 kN."
	)
)
