SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( TM_E242165
	Type ( Engine )
	WagonShape ( TM_E242165.s )
	FreightAnim ( TM_E242165_Detail.s 1 1 )
	Size ( 2.78m 4.53m 16.24m )  
	Mass ( 82.5t )
	WheelRadius ( 0.6m )
	InertiaTensor ( Box ( 2.786m 4.53m 16.26m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 0m 1e9 )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion (  0.2 0.4 2 0 ) 
	DerailRailHeight ( 10cm )
	DerailRailForce ( 207KN )
	DerailBufferForce ( 1000kN )
	NumWheels ( 0 )
	Friction (
		608N/m/s	0	 1mph	      0.35N/m/s  	1.86
		5.1N/rad/s	1	-1rad/s	0		1
	)
	AntiSlip ()

	BrakeEquipmentType( "graduated_release_triple_valve,Auxilary_reservoir,Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 126KN )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 20 )
	MaxApplicationRate( 20 )
	MaxAuxilaryChargingRate( 116 )
	EmergencyResCapacity( 25 )
	EmergencyResChargingRate( 25 )
	EmergencyBrakeResMaxPressure( 72.5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 72.5 )

    	Sound ( "E11Eng.sms" )

	Lights ( 28
	comment ( 12 Lichteinträge für den vorderen Fst, erstellt von Hibu )
            Light	(
			comment( Abblendlicht aussen )
			Type		( 1 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 2 )
			)
			Cycle	( 0 )
			FadeIn	( 0.3 )
			FadeOut	( 0.3 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0 3.0 0 )
					Transition ( 0 )
					Radius ( 80.0 )
					Angle ( 6.0 )
					)
				)
			)
            Light	(
			comment( Fernlicht aussen )
			Type		( 1 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 2 )
			)
			Cycle	( 0 )
			FadeIn	( 0.3 )
			FadeOut	( 0.3 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0 3.25 6.90 )
					Transition ( 0 )
					Radius ( 200.0 )
					Angle ( 4.0 )
					)
				)
			)
		Light	(
			Comment ( Spitzenlicht oben mitte Dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 2 )
			)
			FadeIn	( 0.9 )
			FadeOut	( 1.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0 3.755 7.28 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.15 )
					)
				)
			)
		Light	(
			Comment ( Spitzenlicht oben mitte voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 2 )
			)
			FadeIn	( 0.7 )
			FadeOut	( 0.8 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0 3.755 7.29 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
		Light	(
			Comment ( vorne links Dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 2 )
			)
			FadeIn	( 0.7 )
			FadeOut	( 1.0 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( -0.855 1.975 7.355 )
					Azimuth ( -1.5 -1.5 -1.5 )
					Transition ( 0 )
					Radius ( 0.25 )
					)
				)
			)
		Light	(
			Comment ( vorne links voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 2 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( -0.855 1.975 7.36 )
					Azimuth ( -1 -1 -1 )
					Transition ( 0 )
					Radius ( 0.50 )
					)
				)
			)
		Light	(
			Comment ( vorne rechts Dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 2 )
			)
			FadeIn	( 0.7 )
			FadeOut	( 1.0 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0.86 1.975 7.36 )
					Azimuth ( 1.5 1.5 1.5 )
					Transition ( 0 )
					Radius ( 0.25 )
					)
				)
			)
		Light	(
			Comment ( vorne rechts voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 2 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0.86 1.975 7.365 )
					Azimuth ( 1.5 1.5 1.5 )
					Transition ( 0 )
					Radius ( 0.50 )
					)
				)
			)
		Light	(
			Comment ( Schlusslicht rot links dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 3 )
			)
			FadeIn	( 0.6 )
			FadeOut	( 1.0 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( -0.845 2.255 -7.355 )
					Azimuth ( -178.5 -178.5 -178.5 )
					Transition ( 0 )
					Radius ( 0.15 )
					)
				)
			)
		Light	(
			Comment ( Schlusslicht rot links voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( -0.845 2.255 -7.36 )
					Azimuth ( -178.5 -178.5 -178.5 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
		Light	(
			Comment ( Schlusslicht rot rechts dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 3 )
			)
			FadeIn	( 0.6 )
			FadeOut	( 1.0 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( 0.87 2.255 -7.36 )
					Azimuth ( 178.5 178.5 178.5 )
					Transition ( 0 )
					Radius ( 0.15 )
					)
				)
			)
		Light	(
			Comment ( Schlusslicht rot rechts voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( 0.87 2.255 -7.365 )
					Azimuth ( 178.5 178.5 178.5 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
comment ( 10 Lichteinträge für bin-Patch Cabwechsel in den hinteren Fst erstellt von Hibu )
		Light (
			Comment ( Spitzenlicht oben mitte Dim )
			Type ( 0 )
			Conditions (
			Headlight ( 2 )
			Unit ( 5 )
			)
			FadeIn	( 0.9 )
			FadeOut	( 1.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0 3.755 -7.28 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.15 )
					)
				)
			)
		Light (
			Comment ( Spitzenlicht oben mitte voll )
			Type ( 0 )
			Conditions (
			Headlight ( 3 )
			Unit ( 5 )
			)
			FadeIn	( 0.7 )
			FadeOut	( 0.8 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0 3.755 -7.29 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
		Light	(
			Comment ( vorne links Dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 5 )
			)
			FadeIn	( 0.7 )
			FadeOut	( 1.0 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( -0.855 1.975 -7.36 )
					Azimuth ( -178.5 -178.5 -178.5 )
					Transition ( 0 )
					Radius ( 0.25 )
					)
				)
			)
		Light	(
			Comment ( vorne links voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 5 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( -0.855 1.975 -7.365 )
					Azimuth ( -178.5 -178.5 -178.5 )
					Transition ( 0 )
					Radius ( 0.50 )
					)
				)
			)
		Light	(
			Comment ( vorne rechts Dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 5 )
			)
			FadeIn	( 0.7 )
			FadeOut	( 1.0 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0.86 1.975 -7.36 )
					Azimuth ( 178.5 178.5 178.5 )
					Transition ( 0 )
					Radius ( 0.25 )
					)
				)
			)
		Light	(
			Comment ( vorne rechts voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 5 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0.86 1.975 -7.365 )
					Azimuth ( 178.5 178.5 178.5 )
					Transition ( 0 )
					Radius ( 0.50 )
					)
				)
			)
		Light	(
			Comment ( Schlusslicht rot links dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 4 )
			)
			FadeIn	( 0.6 )
			FadeOut	( 1.0 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( -0.855 2.255 7.355 )
					Azimuth ( -1.5 -1.5 -1.5 )
					Transition ( 0 )
					Radius ( 0.15 )
					)
				)
			)
		Light	(
			Comment ( Schlusslicht rot links voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( -0.855 2.255 7.36 )
					Azimuth ( -1.5 -1.5 -1.5 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
		Light	(
			Comment ( Schlusslicht rot rechts dim )
			Type		( 0 )
			Conditions	(
			Headlight ( 2 )
			Unit ( 4 )
			)
			FadeIn	( 0.6 )
			FadeOut	( 1.0 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( 0.86 2.255 7.355 )
					Azimuth ( 1.5 1.5 1.5 )
					Transition ( 0 )
					Radius ( 0.15 )
					)
				)
			)
		Light	(
			Comment ( Schlusslicht rot rechts voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 3 )
			Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( 0.86 2.255 7.36 )
					Azimuth ( 1.5 1.5 1.5 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
comment( ** blaue Lichtblitze an der Oberleitung ** )
		Light	(
			Type	( 0 ) 
			Conditions	(
			Headlight ( 0 )
			Unit ( 2 )
			Service ( 2 )
			)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 16
				State	(
					Duration ( 0.03 )
					LightColour ( ff0000ff )
					Position ( 0 5.94 -4.25  )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				State	(
					Duration ( 3 )
					LightColour ( 00000000 )
					Position ( 0 3 0  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0 )
					)
				State	(
					Duration ( 0.04 )
					LightColour ( ff87cefa )
					Position ( -0.05 5.94 -4.25  )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				State	(
					Duration ( 7.6 )
					LightColour ( 00000000 )
					Position ( 0 3 0  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0 )
					)
				State	(
					Duration ( 0.1 )
					LightColour ( ff87cefa )
					Position ( 0.025 5.94 -4.25  )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				State	(
					Duration ( 8.3 )
					LightColour ( 00000000 )
					Position ( 0 3 0  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0 )
					)
				State	(
					Duration ( 0.04 )
					LightColour ( ff87cefa )
					Position ( 0 5.94 -4.25  )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( 00000000 )
					Position ( 0 3 0  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( ff0000ff )
					Position ( -0.01 5.94 -4.25  )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				State	(
					Duration ( 6 )
					LightColour ( 00000000 )
					Position ( 0 3 0  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0 )
					)
				State	(
					Duration ( 0.07 )
					LightColour ( ff0000ff )
					Position ( -0.05 5.94 -4.25  )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				State	(
					Duration ( 12 )
					LightColour ( 00000000 )
					Position ( 0 3 0  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( ff87cefa )
					Position ( 0.01 5.94 -4.25  )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				State	(
					Duration ( 0.1 )
					LightColour ( 00000000 )
					Position ( 0 3 0  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0 )
					)
				State	(
					Duration ( 0.03 )
					LightColour ( ff0000ff )
					Position ( -0.01 5.94 -4.25  )
					Azimuth ( 0 -180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
					)
				State	(
					Duration ( 8 )
					LightColour ( 00000000 )
					Position ( 0 3 0  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0 )
					)
				)
			)
comment ( 5 Lichter für Verkehrsloks = KI-Licht erstellt von Hibu )
		Light	(
			comment ( KI Spitzenlicht oben mitte weiss )
			Type		( 0 )
			Conditions	(
			Headlight ( 0 )
			Unit ( 2 )
			Control ( 1 )
			Service ( 2 )
			)
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0 3.755 7.29 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
		Light	(
			Comment ( KI vorne links voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 0 )
			Unit ( 2 )
			Control ( 1 )
			Service ( 2 )
			)
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( -0.855 1.975 7.36 )
					Azimuth ( -1.5 -1.5 -1.5 )
					Transition ( 0 )
					Radius ( 0.50 )
					)
				)
			)
		Light	(
			Comment ( KI vorne rechts voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 0 )
			Unit ( 2 )
			Control ( 1 )
			Service ( 2 )
			)
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffad09f )
					Position ( 0.86 1.975 7.37 )
					Azimuth ( 1.5 1.5 1.5 )
					Transition ( 0 )
					Radius ( 0.50 )
					)
				)
			)
		Light	(
			Comment ( KI Schlusslicht rot links voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 0 )
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			)
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( -0.845 2.255 -7.37 )
					Azimuth ( -178.5 -178.5 -178.5 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
		Light	(
			Comment ( KI Schlusslicht rot rechts voll )
			Type		( 0 )
			Conditions	(
			Headlight ( 0 )
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			)
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( aaff0000 )
					Position ( 0.87 2.255 -7.37 )
					Azimuth ( 178.5 178.5 178.5 )
					Transition ( 0 )
					Radius ( 0.30 )
					)
				)
			)
	      )
)
Engine ( TM_E242165
	Wagon ( TM_E242165 )
	Type ( Electric )
	MaxPower ( 2920kW )
	MaxForce ( 232kN )
	MaxContinuousForce ( 232kN )
	MaxVelocity ( 100kmh )
	MaxCurrent ( 1640A )
	WheelRadius ( 0.675m )
	Sanding ( 20kmh )
	NumWheels ( 4 )

 	CabView ( E11Cab.cvf )
	HeadOut ( 1.79 3.40 5.90 )

	AirBrakesAirCompressorPowerRating ( 3 )
	AirBrakesAirCompressorWattage ( 1000 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.4 )
	AirBrakesCompressorRestartPressure ( 112 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 1 )
	AirBrakesMainMaxAirPressure ( 145 )
	AirBrakesMainMinResAirPressure ( 0 )
	AirBrakesMainResVolume ( 10 )

	EngineBrakesControllerMinPressureReduction ( 6 )
	EngineBrakesControllerMaxApplicationRate ( 20 )
	EngineBrakesControllerMaxReleaseRate ( 30 )
	EngineBrakesControllerEmergencyApplicationRate ( 30 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 72.5 )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	EngineBrakesControllerFullServicePressureDrop ( 72.5 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
      EngineBrakesProportionalBrakeLag( 0.1 )

	TrainBrakesControllerMinPressureReduction ( 5 )
	TrainBrakesControllerMaxApplicationRate ( 10 )
	TrainBrakesControllerMaxReleaseRate ( 20 )
	TrainBrakesControllerEmergencyApplicationRate ( 20 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 72.5 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerFullServicePressureDrop ( 72.5 )

    	DynamicBrakesMinUsableSpeed( 0 )
    	DynamicBrakesMaximumEffectiveSpeed( 0 )
    	DynamicBrakesMaximumForce( 88KN )
    	DynamicBrakesResistorCurrentLimit ( 3600 )
    	DynamicBrakesCutInSpeed( -90 )
    	DynamicBrakesMaxAirBrakePressure ( 54 )
    	DynamicBrakesFadingSpeed( 90 )
    	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
    	DynamicBrakesMaximumSpeedForFadeOut ( 90 )
    	DynamicBrakesEffectAtMaximumFadeOut( 0 )
    	DynamicBrakesHigherSpeedCurveExponent( 1 )
    	DynamicBrakesLowerSpeedCurveExponent( 1 )
    	DynamicBrakesNumberOfControllerNotches( 9 )

	BrakesEngineBrakeType ( Air_single_pipe )
	BrakesTrainBrakeType ( Air_single_pipe )
	BrakesEngineControllers( "Independent,Train,Dynamic" )

	BrakeCutsPowerAtBrakeCylinderPressure ( 14 )
	DoesBrakeCutPower ( 1 )
	DoesHornTriggerBell ( 0 )

	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 45 )
		MonitoringDeviceAlarmTimeLimit ( 37 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 100 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
	)
	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 100 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 79 )
		MonitoringDeviceResetLevel ( 79 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
		MonitoringDeviceResetOnResetButton ( 1 )
		MonitoringDeviceResetOnZeroSpeed ( 0 )
		)
    EngineControllers (
            Throttle ( 0 1 0.2 0 
            NumNotches ( 15
            Notch( 0.00  0 Dummy )
            Notch( 0.07  0 Dummy )
            Notch( 0.14  0 Dummy )
            Notch( 0.21  0 Dummy )
            Notch( 0.28  0 Dummy )
            Notch( 0.35  0 Dummy )
            Notch( 0.42  0 Dummy )
            Notch( 0.49  0 Dummy )
            Notch( 0.56  0 Dummy )
            Notch( 0.63  0 Dummy )
            Notch( 0.70  0 Dummy )
            Notch( 0.77  0 Dummy )
            Notch( 0.84  0 Dummy )
            Notch( 0.91  0 Dummy )
            Notch( 1.00  0 Dummy )
      	)
      )
	Brake_Engine ( 0 1 0.03 0
		NumNotches ( 1
		Notch ( 0 1 Dummy )
		)
	)
	Brake_Train ( 0 1 0.03 0.22
		NumNotches ( 4
		Notch ( 0.00 0 TrainBrakesControllerReleaseStart )
		Notch ( 0.20 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
		Notch ( 0.90 0 TrainBrakesControllerContinuousServiceStart )
		Notch ( 1.00 0 TrainBrakesControllerEmergencyStart )
		)
	)
      Brake_Dynamic ( 0 1 0.06 0 
            NumNotches ( 9
                  Notch ( 0.000  0 Dummy )
                  Notch ( 0.125  0 Dummy )
                  Notch ( 0.250  0 Dummy )
                  Notch ( 0.375  0 Dummy )
                  Notch ( 0.500  0 Dummy )
                  Notch ( 0.625  0 Dummy )
                  Notch ( 0.750  0 Dummy )
                  Notch ( 0.875  0 Dummy )
                  Notch ( 1.000  0 Dummy )
      		)
      )
	DirControl ( -1 0 1 1 )
	EmergencyStopToggle ( 0 1 0 )
	EmergencyStopResetToggle ( 0 1 0 )
	PantographToggle1 ( 0 1 0 )
	PantographToggle2 ( 0 1 0 )
	Headlights ( 0 0.25 1 0 )
	Horn ( 0 1 0 )
	BellToggle ( 0 1 0 )
	Sanding ( 0 1 0 )
      Wipers ( 0 1 0 )
	Vigilance ( 0 1 0 )
	)
    	Sound ( "E11Cab_14stufen.sms" )
    	Name ( "TM_E242 165-9 BW Leipzig/West" )
	Description (
	"Die bei LEW Henningsdorf in Auftrag gegebenen E42 wurden in mehreren Serien geliefert um den grossen "+
	"Bedarf an neuen Loks zu decken.\n\n"+
	"Lokomotivtyp: elektrische Güterzuglokomotive \n\n"+
	"Dauerleistung  : 2760 Kilowatt\n\n"+
	"Stundenleistung: 2920 Kilowatt\n\n"+
	"Höchstgeschwindigkeit: 100 km/h \n\n"+
	"Gewicht: 82,5 t" )
    	EngineOperatingProcedures ( ""
    	)
)
