SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( TM_DBmu_ocker
	comment( Kank verze 1.0 MSTS BIN )
	Type ( Carriage )
	Name ( "TM_DR DBmu_ocker Rbd Dresden" )
	WagonShape ( "TM_DBmu_ocker.s" )
	Size ( 2.835m 4.631m 26.561m )
	CentreOfGravity ( 0m 0m 0m )
	Mass ( 49t )
	WheelRadius ( 46cm )
	InertiaTensor ( Box ( 2.835m 4.631m 26.561m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5E6N/m 1E7N/m )
			Damping ( 1E6N/m/s 2E6N/m/s )
			Break ( 1.1E7N 5E7N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection (  )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5E6N/m 1E7N/m )
			Damping ( 1E6N/m/s 2E6N/m/s )
			Break ( 1.1E7N 5E7N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection (  )
		Velocity ( 0.01m/s )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 125kN )
	DerailBufferForce ( 350kN )
	NumWheels ( 4 )
	Friction (
		834.7N/m/s	-0.1	1.1mph	3.237N/m/s	1.803
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	
 	)

	BrakeEquipmentType ( "handbrake,graduated_release_triple_valve,auxilary_reservoir,emergency_brake_reservoir" )
	BrakeSystemType ( Air_single_pipe )
	MaxBrakeForce ( 60kN )
	EmergencyBrakeResMaxPressure ( 73 )
	TripleValveRatio ( 1.24 )
	MaxReleaseRate ( 1.5 )
	MaxApplicationRate ( 1.5 )
	MaxAuxilaryChargingRate ( 5 )
	EmergencyResCapacity ( 7 )
	EmergencyResChargingRate ( 30 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 35 )
	MaxHandbrakeForce ( 18kN )
	NumberOfHandbrakeLeverSteps ( 100 )
	
	      Sound ( "H_Eilzugwag.sms" )
Inside (
              	PassengerCabinFile ( Bmoint.s )
              	PassengerCabinHeadPos ( 0.95 1.6 0.3 )
              	RotationLimit ( 20 90 20 )
              	StartDirection ( 0 0 0 )
		Sound ("H_Eilzugwag.sms" )
	)

	Lights ( 6
		Light	(
			comment( rechts abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					LightColour ( ffff0000 )
					Position ( 0.9 1.86 -13.22 )
					Azimuth ( 180 180 180 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( links abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					LightColour ( ffff0000 )
					Position ( -0.9 1.86 -13.22 )
					Azimuth ( 180 180 180 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( rechts voll )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					LightColour ( ffff0000 )
					Position ( 0.9 1.86 -13.22 )
					Azimuth ( 180 180 180 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( links voll )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					LightColour ( ffff0000 )
					Position ( -0.9 1.86 -13.22 )
					Azimuth ( 180 180 180 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( KI rechts )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Service ( 2 )
				Control ( 1 )
			)
			States ( 1
				State	(
					LightColour ( ffff0000 )
					Position ( 0.9 1.86 -13.22 )
					Azimuth ( 180 180 180 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( KI links )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Service ( 2 )
				Control ( 1 )
			)
			States ( 1
				State	(
					LightColour ( ffff0000 )
					Position ( -0.9 1.86 -13.22 )
					Azimuth ( 180 180 180 )
					Radius ( 0.4 )
				)
			)
		)
	)

)