SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( H-START_61_55_21-91_332-2_Bvmz
	Type ( Carriage )
	Name ( "H-START DWA-Pack 332-2 Bvmz" )
	WagonShape ( H-START_61_55_21-91_332-2_Bvmz.s )
	FreightAnim ( H-START_61_55_21-91_332-2_Bvmz_freight.s 1 1 )
	Size ( 2.974m 4.075m 26.402m)
	CentreOfGravity ( 0m 0.1m 0m )
	Mass ( "42t" )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box (2.974m 4.075m 26.402m) )
	comment	( Coupling )

comment ( Rear Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
	CouplingHasRigidConnection ( 0 )
	Velocity ( 0.01m/s )
	)
	
comment ( Front Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
        CouplingHasRigidConnection ( 0 )
        Velocity ( 0.01m/s )
	)

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 2.5*27t )
	DerailBufferForce ( 400kN )
	NumWheels (8 )
	Friction (
		100N/m/s		1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s		0		1
	)

	
            Inside (
            PassengerCabinFile      ( H-START_61_55_21-91_332-2_Bvmz.s )
            PassengerCabinHeadPos ( -.93 2.4 -.825 )
            RotationLimit ( 40 180 0 )
            StartDirection ( 0 0 0 )
            Sound ( "..\\..\\MAV_Hangok\\Intercity\\DZUGALT_IN.sms" )    
	)
Lights	(10		
		Light	(
			comment( postojowe prawe )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( .99 1.76 -12.96 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.40 )
				)
			)
		)
		Light	(
			comment( pelne prawe )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( .99 1.76 -12.96 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.65 )
				)
			)
		)
		Light	(
			comment( postojowe lewe )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -.99 1.76 -12.96 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.40 )
				)
			)
		)
		Light	(
			comment( pelne lewe )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -.99 1.76 -12.96 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.65 )
				)
			)
		)
	       Light	(
			comment( postojowe lewe R )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( .99 1.76 12.96 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.40 )
				)
			)
		)
		Light	(
			comment( pelne lewe R )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( .99 1.76 12.96 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.65 )
				)
			)
		)
		Light	(
			comment( postojowe prawe R )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -.99 1.76 12.96 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.40 )
				)
			)
		)
		Light	(
			comment( pelne prawe R )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -.99 1.76 12.96 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.65 )
				)
			)
		)
		Light	(
			comment( pelne prawe AI )
			Type		( 0 )
			Conditions (
    			  Control ( 1 )
			  Unit ( 3 )
  			  Service ( 2 )
 			  TimeOfDay ( 0 )
 			   )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( .99 1.76 -12.96 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.65 )
				)
			)
		)
		Light	(
			comment( pelne lewe AI )
			Type		( 0 )
			Conditions (
    			  Control ( 1 )
			  Unit ( 3 )
 			  Service ( 2 )
 			  TimeOfDay ( 0 )
			   )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -.99 1.76 -12.96 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.65 )
				)
			)
		)


	)	
	BrakeEquipmentType( "Handbrake, Graduate_release_Triple_valve, Auxilary_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 42kN )

	MaxHandbrakeForce( 21kN )
	NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 3 )
	MaxApplicationRate( 10.5 )
	MaxAuxilaryChargingRate( 3 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 11 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 ) 

  	Sound ( "..\\..\\MAV_Hangok\\Intercity\\DZUG140.sms" )
)