SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( H-START_88-71_003-3_WRbumz 
 Type ( Carriage )
 Name ("H-START DWA-Pack 003-3 WRbumz")
 WagonShape ( H-START_88-71_003-3_WRbumz.s )
 comment( Semora uprava pro TrainsetBP a nastavení chování )
        Size ( 2.91m 4.052m 26.413m )
 CentreOfGravity ( 0m 1.9m 0m )
 Mass ( 38t )
 WheelRadius ( 0.46m )
 InertiaTensor ( Box (2.91m 4.052m 26.413m) )
 comment	( Coupling )

comment ( Rear Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
	CouplingHasRigidConnection ( 0 )
	Velocity ( 0.01m/s )
	)
	
comment ( Front Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
        CouplingHasRigidConnection ( 0 )
        Velocity ( 0.01m/s )
	)

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
 Adheasion ( 0.2 0.4 2 0 )
 DerailRailHeight ( 10cm )
 DerailRailForce ( 2.5*41t )
 DerailBufferForce ( 350kN )
 NumWheels ( 4 )
 Friction (
  777.3N/m/s  -0.1  1.2mph  2.704N/m/s  1.799
  5.1N/rad/s  1  -1rad/s  0  1
 )


 Lights ( 10
    
  Light (
   comment( Rear red light dim )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.985 2.037 -13.08 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
	Light (
   comment( Rear red light dim kabincsere )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 4 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.985 2.037 13.08 )
     Azimuth ( 0 0 0 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )

  Light (
   comment( Rear red light bright )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.985 2.037 -13.08 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
 Light (
   comment( Rear red light bright kabincsere )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 4 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.985 2.037 13.08 )
     Azimuth ( 0 0 0 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )

  Light (
   comment( Rear red light dim )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( -0.985 2.037 -13.08 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
 Light (
   comment( Rear red light dim kabincsere )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 4 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( -0.985 2.037 13.08 )
     Azimuth ( 0 0 0 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )

  Light (
   comment( Rear red light bright )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( -0.985 2.037 -13.08 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
Light (
   comment( Rear red light bright kabincsere )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 4 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( -0.985 2.037 13.08 )
     Azimuth ( 0 0 0 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
 Light (
   comment( Rear red light bright AI )
   Type  ( 0 )
   Conditions (
    Control ( 1 )
    Unit ( 3 )
    Service ( 2 )
    TimeOfDay ( 0 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( -0.985 2.037 -13.08 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
 Light (
   comment( Rear red light bright AI )
   Type  ( 0 )
   Conditions (
      Control ( 1 )
	Unit ( 3 )
	Service ( 2 )
	TimeOfDay ( 0 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.985 2.037 -13.08 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )


 )

 BrakeEquipmentType ( "Handbrake, Graduate_release_Triple_valve, Auxilary_reservoir" )
 BrakeSystemType ( "Air_single_pipe" )
 MaxBrakeForce( 59kN )

 MaxHandbrakeForce( 9kN )
 NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 3 )
	MaxApplicationRate( 10.5 )
	MaxAuxilaryChargingRate( 3 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 11 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 ) 

 Sound ( "..\\..\\MAV_Hangok\\Intercity\\DZUG140.sms" )
)
