SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_Ampz_002
	Type ( Carriage )
	Name ("CD vuz Ampz 002")
	WagonShape ( cd_Ampz_002.s )
	Size ( 2.89m 4.12m 25.79m )
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 51t )
	WheelRadius ( 0.46m )
	InertiaTensor ( Box (2.89m 4.12m 25.79m) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 80cm 150cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*49t )
	DerailBufferForce ( 350kN )
	NumWheels ( 4 )
	Friction (
		738.2N/m/s  -0.05  1.0mph  2.418N/m/s  1.819
		5.1N/rad/s  1  -1rad/s  0  1
	)
	Lights ( 10
		Light	(
			comment( hrac normal predni pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 13.08 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac normal predni levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 13.08 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac normal zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac normal zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac otocene predni pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 4 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 13.08 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac otocene predni levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 4 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 13.08 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac otocene zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( hrac otocene zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( trf normal zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( trf normal zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.24 2.12 -13.08 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)

	BrakeEquipmentType ( "Handbrake, Graduated_release_Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
      BrakeSystemType ( "Air_single_pipe" )
      comment( režim P - MaxBrakeForce( 57kN ))
      comment( režim R )
      MaxBrakeForce( 82kN )

      MaxHandbrakeForce( 10kN )
      NumberOfHandbrakeLeverSteps( 100 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 2.2 )
	MaxApplicationRate( 1.7 )
	MaxAuxilaryChargingRate( 3 )
      BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
      EmergencyResVolumeMultiplier ( 11 )
      EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 ) 


  	Sound ( "../../common.snd/vozy/CDvuzOsKlima4nEx.sms" )
)
