SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RJ_ABmz_012
	Type ( Carriage )
	Name ( "RJ_ABmz_012" )
	WagonShape ( RJ_ABmz_012.s )
	Comment ( verze modelu: 1.0 , 15.1.2013 )
        Comment ( brzdy pro Openrails dle navodu od Josefa V. )  
	Size ( 2.91m 4.14m 26.29m )
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 53t )
	WheelRadius ( 0.46m )
	InertiaTensor ( Box ( 2.91m 4.14m 26.29m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

	Comment ( "Jizdni odpory a treni" )

CentreOfGravity ( 0m 2.04m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 2m 60mm )
ORTSUnbalancedSuperelevation ( 150mm )

DerailRailHeight ( 4cm )
DerailRailForce ( 123.5kN )
DerailBufferForce ( 484kN )
ORTSBearingType ( Roller )
ORTSDavis_A ( 830.8 )
ORTSDavis_B ( 16.25 )
ORTSDavis_C ( 0.9041 )

	Lights ( 10
		Light	(
			comment( hrac normal predni pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.893 2.090 13.074 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( hrac normal predni levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.995 2.080 13.074 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( hrac normal zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.935 2.13 -13.074 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( hrac normal zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.934 2.13 -13.074 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( hrac otocene predni pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 4 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.893 2.090 13.074 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( hrac otocene predni levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 4 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.995 2.080 13.074 )
					Azimuth ( 0.25 0.0 0.25 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( hrac otocene zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.935 2.13 -13.074 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( hrac otocene zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.934 2.13 -13.074 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( trf normal zadní pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.935 2.13 -13.074 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( trf normal zadní levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Service ( 2 )
				Control ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.934 2.13 -13.074 )
					Azimuth ( -155 180 -155 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
	)

	Comment ( "Brzdy" )
        Comment ( "Brzdovy system DAKO, kotouce, Bv.P: 53t" )
        Comment ( "Rezim brzdeni P")
        BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
        BrakeSystemType ( "Air_single_pipe" )

        MaxBrakeForce ( 165kN )
        MaxHandbrakeForce ( 40kN )
        NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.2bar/s )
MaxApplicationRate ( 0.45bar/s )
MaxAuxilaryChargingRate ( 1.013bar/s )
EmergencyResChargingRate ( 1.013bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 3.8bar )
EmergencyResVolumeMultiplier ( 1.0 )
EmergencyResCapacity ( 120l )
BrakePipeVolume ( 22l )

ORTSBrakeShoeFriction ( 0 0.420 1 0.408 2 0.390 3 0.380 4 0.370 5 0.360 7 0.345 8 0.340 9 0.332 12 0.319 14 0.309 16 0.300 20 0.290 24 0.280 30 0.268 34 0.260 40 0.250 48 0.236 56 0.222 68 0.209 84 0.200 120 0.200 160 0.200 ) 

  	Sound ( "..//..//common.snd//sndVozy//CDvuzOsVetr4nEx-OR.sms" )
)
